IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-10-15T16:16:50"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.0.490.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "stud5342" of Organization (no name given)
  Owner history of Person "stud5342" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1443527864 (2015-09-29T11:57:44Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation -500.000000000001
        contains 19 elements
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:295 mm betonfundament" | object type "Basic Wall:295 mm betonfundament:311141" | names: "Basic Wall:295 mm betonfundament:311920", "Basic Wall:295 mm betonfundament:312005", "Basic Wall:295 mm betonfundament:312083" (+10 more) | material: layers "Basic Wall:295 mm betonfundament" ("Concrete, Cast In Situ" 295.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys inne høy" | object type "ovenlys inne høy" | names: "M_Fixed:ovenlys inne høy:339405" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys inne høy" | object type "ovenlys inne høy" | names: "M_Fixed:ovenlys inne høy:339950", "M_Fixed:ovenlys inne høy:340422", "M_Fixed:ovenlys inne høy:340780" (+1 more) | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCANNOTATION
      IFCBUILDINGSTOREY "Snitt i Plan" | long name "Snitt i Plan" | elevation -5.41433564649196E-13
        contains 52 elements
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:400mm ydervæg" | object type "Basic Wall:400mm ydervæg:313508" | names: "Basic Wall:400mm ydervæg:314850", "Basic Wall:400mm ydervæg:314930", "Basic Wall:400mm ydervæg:315346" (+5 more) | material: layers "Basic Wall:400mm ydervæg" ("Brick, Common" 400.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          14 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:250 mm skilevæg" | object type "Basic Wall:250 mm skilevæg:317488" | names: "Basic Wall:250 mm skilevæg:315578", "Basic Wall:250 mm skilevæg:315913", "Basic Wall:250 mm skilevæg:316364" (+11 more) | material: layers "Basic Wall:250 mm skilevæg" ("Default Wall" 250.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:400mm skilevæg 2" | object type "Basic Wall:400mm skilevæg 2:346889" | names: "Basic Wall:400mm skilevæg 2:321674", "Basic Wall:400mm skilevæg 2:345707", "Basic Wall:400mm skilevæg 2:347586" | material: layers "Basic Wall:400mm skilevæg 2" ("Default Wall" 400.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "72_vindu" | object type "72_vindu" | names: "M_Fixed:72_vindu:323246", "M_Fixed:72_vindu:332610" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "72_vindu 2 extra long" | object type "72_vindu 2 extra long" | names: "M_Fixed:72_vindu 2 extra long:325708" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "72 door wide" | object type "72 door wide" | names: "M_Single-Flush:72 door wide:326930", "M_Single-Flush:72 door wide:328299", "M_Single-Flush:72 door wide:328565" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCDOOR | type IFCDOORSTYLE "0762 x 2032mm" | object type "0762 x 2032mm" | names: "M_Single-Flush:0762 x 2032mm:327666", "M_Single-Flush:0762 x 2032mm:327734", "M_Single-Flush:0762 x 2032mm:334129" (+1 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          3 x IFCDOOR | type IFCDOORSTYLE "0813 x 2134mm" | object type "0813 x 2134mm" | names: "M_Single-Flush:0813 x 2134mm:327875", "M_Single-Flush:0813 x 2134mm:329178", "M_Single-Flush:0813 x 2134mm:329292" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          8 x IFCDOOR | type IFCDOORSTYLE "0864 x 2032mm" | object type "0864 x 2032mm" | names: "M_Single-Flush:0864 x 2032mm:327982", "M_Single-Flush:0864 x 2032mm:328065", "M_Single-Flush:0864 x 2032mm:328185" (+5 more) | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "0864 x 2032mm" | object type "0864 x 2032mm" | names: "M_Single-Flush:0864 x 2032mm:328916" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:331530" | material: layers "Floor:Generic 300mm" ("Default Floor" 300.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "0915 x 2032mm" | object type "0915 x 2032mm" | names: "M_Single-Flush:0915 x 2032mm:333649" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "Great Door" | object type "Great Door" | names: "M_Single-Flush:Great Door:333982" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:sæylevegg" | object type "Basic Wall:sæylevegg:320221" | names: "Basic Wall:sæylevegg:345097" | material: layers "Basic Wall:sæylevegg" ("Default Wall" 250.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:500mmk skilevæg 3" | object type "Basic Wall:500mmk skilevæg 3:347828" | names: "Basic Wall:500mmk skilevæg 3:347879" | material: layers "Basic Wall:500mmk skilevæg 3" ("Default Wall" 500.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
      IFCBUILDINGSTOREY "Bottom windows" | long name "Bottom windows" | elevation 959.999999999999
        contains 29 elements
          20 x IFCWINDOW | type IFCWINDOWSTYLE "72_vindu" | object type "72_vindu" | names: "M_Fixed:72_vindu:321802", "M_Fixed:72_vindu:322729", "M_Fixed:72_vindu:322859" (+17 more) | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys inne lav" | object type "ovenlys inne lav" | names: "M_Fixed:ovenlys inne lav:341255", "M_Fixed:ovenlys inne lav:341621" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys inne høy" | object type "ovenlys inne høy" | names: "M_Fixed:ovenlys inne høy:341827", "M_Fixed:ovenlys inne høy:341935", "M_Fixed:ovenlys inne høy:341999" (+1 more) | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys inne høy" | object type "ovenlys inne høy" | names: "M_Fixed:ovenlys inne høy:343482" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "ovenlys køkken 762" | object type "ovenlys køkken 762" | names: "M_Fixed:ovenlys køkken 762:348303", "M_Fixed:ovenlys køkken 762:348920" | material: materials ("Glass", "Sash") | property sets: Pset_WindowCommon, Constraints, Dimensions, Identity Data, Other, Phasing
      IFCBUILDINGSTOREY "Top window indoor" | long name "Top window indoor" | elevation 2950.
        contains 4 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:sæylevegg" | object type "Basic Wall:sæylevegg:320221" | names: "Basic Wall:sæylevegg:345565", "Basic Wall:sæylevegg:345997", "Basic Wall:sæylevegg:346682" (+1 more) | material: layers "Basic Wall:sæylevegg" ("Default Wall" 250.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | elevation 3199.99999999984
        contains 1 element
          1 x IFCSLAB | object type "Floor:Generic 300mm" | FLOOR | names: "Floor:Generic 300mm:349636" | material: layers "Floor:Generic 300mm" ("Default Floor" 300.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural

Types
  IFCWALLTYPE "Basic Wall:295 mm betonfundament" | STANDARD | 13 occurrences | material: layers "Basic Wall:295 mm betonfundament" ("Concrete, Cast In Situ" 295.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWINDOWSTYLE "ovenlys inne høy" | 2 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:ovenlys inne høy:339405, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "ovenlys inne høy" | 8 occurrences | material: materials ("Glass", "Sash") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:400mm ydervæg" | STANDARD | 8 occurrences | material: layers "Basic Wall:400mm ydervæg" ("Brick, Common" 400.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:250 mm skilevæg" | STANDARD | 14 occurrences | material: layers "Basic Wall:250 mm skilevæg" ("Default Wall" 250.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:400mm skilevæg 2" | STANDARD | 3 occurrences | material: layers "Basic Wall:400mm skilevæg 2" ("Default Wall" 400.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "72_vindu" | 22 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:72_vindu:321802, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "72_vindu 2 extra long" | 1 occurrence | material: materials ("Glass", "Sash") | property sets: M_Fixed:72_vindu 2 extra long:325708, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "72 door wide" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:72 door wide:326930, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "0762 x 2032mm" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0762 x 2032mm:327666, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "0813 x 2134mm" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "0864 x 2032mm" | SINGLE_SWING_RIGHT | 8 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "0864 x 2032mm" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "0915 x 2032mm" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: M_Single-Flush:0915 x 2032mm:333649, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "Great Door" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:sæylevegg" | STANDARD | 5 occurrences | material: layers "Basic Wall:sæylevegg" ("Default Wall" 250.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:500mmk skilevæg 3" | STANDARD | 1 occurrence | material: layers "Basic Wall:500mmk skilevæg 3" ("Default Wall" 500.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWINDOWSTYLE "ovenlys inne lav" | 2 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:ovenlys inne lav:341255, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWINDOWSTYLE "ovenlys køkken 762" | 2 occurrences | material: materials ("Glass", "Sash") | property sets: M_Fixed:ovenlys køkken 762:348303, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes

Property sets
  Constraints | properties | on 27 objects (27 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Snitt i Plan" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3199.99999999984 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 25 objects (21 IFCDOOR, 4 IFCOPENINGELEMENT)
    Level = "Level: Snitt i Plan" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 13 objects (13 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Snitt i Plan" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 500. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 11 objects (11 IFCWINDOW)
    Level = "Level: Bottom windows" (IFCLABEL)
    Sill Height = -29.9999999999999 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 8 objects (8 IFCWINDOW)
    Level = "Level: Bottom windows" (IFCLABEL)
    Sill Height = -30. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 6 objects (6 IFCWINDOW)
    Level = "Level: Bottom windows" (IFCLABEL)
    Sill Height = 1429.99999999984 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Top window indoor" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Finish Face: Interior" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 249.999999999837 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 16 more contents on 19 objects not shown
  Dimensions | properties | on 22 objects (22 IFCWINDOW)
    Area = 4.98252400000013 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.10297018 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 10 objects (9 IFCDOOR, 1 IFCOPENINGELEMENT)
    Area = 2.93330399999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.108842047999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 10 objects (10 IFCWINDOW)
    Area = 2.33144400000009 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0468006399999989 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 5 objects (3 IFCDOOR, 2 IFCOPENINGELEMENT)
    Area = 2.94610499999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.108367441999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 4 objects (4 IFCDOOR)
    Area = 2.70023399999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0978839839999994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 3 objects (3 IFCDOOR)
    Area = 3.22538399999998 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.121545619999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 2 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT)
    Area = 4.44807399999997 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.175824599999999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 61 more contents on 52 objects not shown
  Other | properties | on 20 objects (20 IFCWINDOW)
    Category = "Windows" (IFCLABEL)
    Family = "M_Fixed: 72_vindu" (IFCLABEL)
    Family and Type = "M_Fixed: 72_vindu" (IFCLABEL)
    Head Height = 1770. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 400mm ydervæg" (IFCLABEL)
    Type = "M_Fixed: 72_vindu" (IFCLABEL)
    Type Id = "M_Fixed: 72_vindu" (IFCLABEL)
  Other | properties | on 14 objects (14 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
    Family and Type = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
    Type = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
    Type Id = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
  Other | properties | on 13 objects (13 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 295 mm betonfundament" (IFCLABEL)
    Family and Type = "Basic Wall: 295 mm betonfundament" (IFCLABEL)
    Type = "Basic Wall: 295 mm betonfundament" (IFCLABEL)
    Type Id = "Basic Wall: 295 mm betonfundament" (IFCLABEL)
  Other | properties | on 10 objects (9 IFCDOOR, 1 IFCOPENINGELEMENT)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: 0864 x 2032mm" (IFCLABEL)
    Family and Type = "M_Single-Flush: 0864 x 2032mm" (IFCLABEL)
    Head Height = 2032. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
    Type = "M_Single-Flush: 0864 x 2032mm" (IFCLABEL)
    Type Id = "M_Single-Flush: 0864 x 2032mm" (IFCLABEL)
  Other | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: 400mm ydervæg" (IFCLABEL)
    Family and Type = "Basic Wall: 400mm ydervæg" (IFCLABEL)
    Type = "Basic Wall: 400mm ydervæg" (IFCLABEL)
    Type Id = "Basic Wall: 400mm ydervæg" (IFCLABEL)
  Other | properties | on 5 objects (3 IFCDOOR, 2 IFCOPENINGELEMENT)
    Category = "Doors" (IFCLABEL)
    Family = "M_Single-Flush: 0813 x 2134mm" (IFCLABEL)
    Family and Type = "M_Single-Flush: 0813 x 2134mm" (IFCLABEL)
    Head Height = 2134. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: 250 mm skilevæg" (IFCLABEL)
    Type = "M_Single-Flush: 0813 x 2134mm" (IFCLABEL)
    Type Id = "M_Single-Flush: 0813 x 2134mm" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: sæylevegg" (IFCLABEL)
    Family and Type = "Basic Wall: sæylevegg" (IFCLABEL)
    Type = "Basic Wall: sæylevegg" (IFCLABEL)
    Type Id = "Basic Wall: sæylevegg" (IFCLABEL)
  Other | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other: 23 more contents on 42 objects not shown
  Phasing | properties | on 108 objects (44 IFCWALLSTANDARDCASE, 37 IFCWINDOW, 21 IFCDOOR, 4 IFCOPENINGELEMENT)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 44 objects (44 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 2 objects (2 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 14 objects (14 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "250 mm skilevæg" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 13 objects (13 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "295 mm betonfundament" (IFCIDENTIFIER)
    ThermalTransmittance = 3.54576271186441 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "400mm ydervæg" (IFCIDENTIFIER)
    ThermalTransmittance = 1.35 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "sæylevegg" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "400mm skilevæg 2" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "500mmk skilevæg 3" (IFCIDENTIFIER)
  Identity Data | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 3 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT, 1 IFCWINDOW)
    Mark = "19" (IFCTEXT)
  Identity Data | properties | on 3 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT, 1 IFCWINDOW)
    Mark = "18" (IFCTEXT)
  Identity Data | properties | on 3 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT, 1 IFCWINDOW)
    Mark = "22" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCOPENINGELEMENT)
    Mark = "17" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCDOOR, 1 IFCWINDOW)
    Mark = "5" (IFCTEXT)
  Identity Data: 63 more contents on 54 objects not shown
  Pset_WindowCommon | properties | on 22 objects (22 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "72_vindu" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 10 objects (10 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ovenlys inne høy" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ovenlys inne lav" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "ovenlys køkken 762" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "72_vindu 2 extra long" (IFCIDENTIFIER)
    ThermalTransmittance = 3.6886 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 9 objects (9 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0864 x 2032mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0762 x 2032mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "72 door wide" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0813 x 2134mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "0915 x 2032mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Great Door" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 300mm" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 5 (IFCINTEGER)
  Analytical Properties | properties | on 2 objects (2 IFCSLAB) | on 4 type objects
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Analytical Properties | properties | on 7 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 6 type objects
    Analytic Construction = "1/8 in Pilkington single glazing" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.6886 (IFCREAL)
    Solar Heat Gain Coefficient = 0.78 (IFCREAL)
    Thermal Resistance (R) = 0.271105568508377 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 3.54576271186441 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.282026768642447 (IFCREAL)
    Thermal mass = 445774.5 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 1.35 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.740740740740741 (IFCREAL)
    Thermal mass = 520800. (IFCREAL)
  Construction | properties | on 2 objects (2 IFCSLAB)
    Default Thickness = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 7 type objects
    Function = "Interior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 6 type objects
    Wall Closure = "By host" (IFCIDENTIFIER)
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 2 type objects
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 295. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Graphics | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 2 objects (2 IFCSLAB) | on 6 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Materials and Finishes | properties | on 7 type objects
    Door Material = "Door - Panel" (IFCLABEL)
    Frame Material = "Door - Frame" (IFCLABEL)
  Materials and Finishes | properties | on 6 type objects
    Frame Exterior Material = "Sash" (IFCLABEL)
    Frame Interior Material = "Sash" (IFCLABEL)
    Glass Pane Material = "Glass" (IFCLABEL)
    Sash = "Sash" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "Concrete, Cast In Situ" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "Brick, Common" (IFCLABEL)
  M_Fixed:ovenlys inne høy:339405 | predefined | on 1 type object
  M_Fixed:ovenlys inne høy:339950 | predefined | on 1 type object
  M_Fixed:72_vindu:321802 | predefined | on 1 type object
  M_Fixed:72_vindu 2 extra long:325708 | predefined | on 1 type object
  M_Single-Flush:72 door wide:326930 | predefined | on 2 type objects
  M_Single-Flush:0762 x 2032mm:327666 | predefined | on 2 type objects
  M_Single-Flush:0813 x 2134mm:327875 | predefined | on 2 type objects
  M_Single-Flush:0864 x 2032mm:327982 | predefined | on 2 type objects
  M_Single-Flush:0864 x 2032mm:328916 | predefined | on 2 type objects
  M_Single-Flush:0915 x 2032mm:333649 | predefined | on 2 type objects
  M_Single-Flush:Great Door:333982 | predefined | on 2 type objects
  M_Fixed:ovenlys inne lav:341255 | predefined | on 1 type object
  M_Fixed:ovenlys køkken 762:348303 | predefined | on 1 type object