IFC building model
Schema: "IFC2X2_FINAL"
Description: "IFC2X2_FINAL"
File name: "HiB_PipeWork.ifc"
Time stamp: "2005-04-01T14:30:13"
Author: "ST"
Organization: "Data Design System ASA"
Preprocessor: "DDS-IFC v1.0"
Originating system: "Building Services Partner Version 6.35 Prerel build 1/4-2005"
Authorization: "DDS"
Application: "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS"
Application: "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS"
Application: "Common Building functions Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Common Building functions" by Organization "DDS"
Application: "PipeWork Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "PipeWork" by Organization "DDS"

People and organizations
  4 x Person "Stian" "Tonheim" of Organization "DDS"
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS" | change NOCHANGE | created 1112354092 (2005-04-01T11:14:52Z)
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS" | change NOCHANGE | created 1112358506 (2005-04-01T12:28:26Z)
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "PipeWork Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "PipeWork" by Organization "DDS" | change NOCHANGE | created 1112358523 (2005-04-01T12:28:43Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  MASSUNIT: GRAM
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICRESISTANCEUNIT: OHM
  POWERUNIT: WATT
  MASSUNIT: GRAM
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  PRESSUREUNIT: PASCAL
  LUMINOUSFLUXUNIT: LUMEN
  ILLUMINANCEUNIT: LUX
  VOLUMEUNIT: CUBIC_METRE
  TIMEUNIT: SECOND
  VOLUMETRICFLOWRATEUNIT: derived

Spatial structure
IFCPROJECT "DDS Project"
  IFCSITE | postal address: "Bergen"
    IFCBUILDING | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Ventilation in ground" | COMPLEX | elevation 0. | description "Ventilation in ground"
        contains 1266 elements
          29 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3" ( 88.9X4.0) steel pipe DN 80" ("ML-3" ( 88.9X4.0) steel pipe DN 80" 0.004) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          25 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          818 x IFCDISTRIBUTIONPORT
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          27 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-4" (114.3X4.5) steel pipe DN 100" ("ML-4" (114.3X4.5) steel pipe DN 100" 0.004500000000000001) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          23 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          19 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-75MMX3.0M PP drain pipe" ("ML-75MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          68 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-110MMX6,0M PP drain pipe" ("ML-110MMX6,0M PP drain pipe" 0.004500000000000001) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          66 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          75 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-110MMX3.0M PP drain pipe" ("ML-110MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          16 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          24 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-160MMX6,0M PP drain pipe" ("ML-160MMX6,0M PP drain pipe" 0.004500000000000001) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          5 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "GU2104" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
      IFCBUILDINGSTOREY "Ventilation basement" | COMPLEX | elevation 0. | description "Ventilation basement"
        contains 3490 elements
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2152" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2151" | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCWASTETERMINALTYPE "GU2101" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2900" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2153" | property sets: Pset_Draughting
          5 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-54 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-54 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2316 x IFCDISTRIBUTIONPORT
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "BD2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          9 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-42 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-42 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          14 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          9 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          21 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_FlowSegmentPipeSegment, Pset_Draughting
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          24 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" 0.0015, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          58 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          17 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" 0.001, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          34 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          7 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          50 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          8 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          15 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" 0.002) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 1,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-12 X 1,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.001, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          43 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-110MMX3.0M PP drain pipe" ("ML-110MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          14 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-50MMX3,0M PP drain pipe" ("ML-50MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          7 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-75MMX3.0M PP drain pipe" ("ML-75MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          13 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-32MMX3,0M PP drain pipe" ("ML-32MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          12 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          10 x IFCBUILDINGELEMENTPROXY | names: "Heater" | property sets: Pset_Draughting
          61 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32" 0.003200000047683716); layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          4 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          29 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          4 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/2" ( 48.3X3.2) steel pipe DN 40-Mineral wool 50 mm-50" ("ML-11/2" ( 48.3X3.2) steel pipe DN 40-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          21 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          20 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1" ( 33.7X3.2) steel pipe DN 25-Mineral wool 50 mm-50" ("ML-1" ( 33.7X3.2) steel pipe DN 25-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          5 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          4 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          26 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          74 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          13 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          103 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          88 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" ("ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          7 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          33 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          8 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/2" ( 48.3X3.2) steel pipe DN 40 cold water-Mineral wool 50 mm-50" ("ML-11/2" ( 48.3X3.2) steel pipe DN 40 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          14 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32 cold water-Mineral wool 50 mm-50" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          24 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" ("ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          14 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1/2" ( 21.3X2.6) steel pipe DN 15-Mineral wool 50 mm-50" ("ML-1/2" ( 21.3X2.6) steel pipe DN 15-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
      IFCBUILDINGSTOREY "Ventilation 1th floor" | COMPLEX | elevation 2.75 | description "Ventilation 1th floor"
        contains 2911 elements
          5 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2152" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2151" | property sets: Pset_Draughting
          3 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | property sets: Pset_Draughting
          14 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" 0.001, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1904 x IFCDISTRIBUTIONPORT
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          19 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          50 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          57 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          48 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          57 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" 0.002); layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water-Mineral wool 20 mm-20" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          21 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" 0.0015, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          9 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          28 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          19 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          13 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          20 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-75MMX3.0M PP drain pipe" ("ML-75MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | property sets: Pset_Draughting
          25 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-32MMX3,0M PP drain pipe" ("ML-32MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2153" | property sets: Pset_Draughting
          21 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-110MMX3.0M PP drain pipe" ("ML-110MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          26 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes cold water-Mineral wool 20 mm-20" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2904" | property sets: Pset_Draughting
          17 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-50MMX3,0M PP drain pipe" ("ML-50MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          8 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          3 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          7 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          18 x IFCBUILDINGELEMENTPROXY | names: "Heater" | property sets: Pset_Draughting
          23 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32" 0.003200000047683716); layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          26 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          10 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32 cold water-Mineral wool 50 mm-50" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          26 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" ("ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          22 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2061" | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          27 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1" ( 33.7X3.2) steel pipe DN 25-Mineral wool 50 mm-50" ("ML-1" ( 33.7X3.2) steel pipe DN 25-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          22 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20" 0.002599999904632569); layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "DI2557" | property sets: Pset_Draughting
          58 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          27 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" ("ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          82 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05); layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water" 0.002599999904632569) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          4 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2061" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          2 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2061" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-4" (114.3X4.5) steel pipe DN 100 cold water" ("ML-4" (114.3X4.5) steel pipe DN 100 cold water" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
      IFCBUILDINGSTOREY "Ventilation 2nd floor" | COMPLEX | elevation 5.5 | description "Ventilation 2nd floor"
        contains 3462 elements
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2902" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCELECTRICAPPLIANCETYPE "WM2001" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2153" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2151" | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          92 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-75MMX3.0M PP drain pipe" ("ML-75MMX3.0M PP drain pipe" 0.004500000000000001); layers "ML-75MMX3.0M PP drain pipe-Mineral wool 50 mm-50" ("ML-75MMX3.0M PP drain pipe-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          20 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2312 x IFCDISTRIBUTIONPORT
          16 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-35 X 2,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-12 X 1,0 cupric pipe hot water-Mineral wool 20 mm-20" 0.001, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          21 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          7 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          13 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-110MMX3.0M PP drain pipe" ("ML-110MMX3.0M PP drain pipe" 0.004500000000000001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-32MMX3,0M PP drain pipe" ("ML-32MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          12 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          77 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-50MMX3,0M PP drain pipe" ("ML-50MMX3,0M PP drain pipe" 0.001) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          37 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          31 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          13 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-18 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          31 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          7 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          6 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-18 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-18 X 1,2 cupric pipe cold water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          22 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes cold water-Mineral wool 20 mm-20" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes cold water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          27 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water-Mineral wool 20 mm-20" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water-Mineral wool 20 mm-20" 0.002, "Layer-Mineral wool 20 mm" 0.02); layers "ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" ("ML-12 X 2.0 mm wirsbo-pex pipe in pipes hot water" 0.002) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-12 X 1,0 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-12 X 1,0 cupric pipe cold water-Mineral wool 20 mm-20" 0.001, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC2152" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "SI2152" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          50 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes cold water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          46 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" ("ML-15 X 2.5 mm wirsbo-pex pipe in pipes hot water" 0.0025) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          6 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" ("ML-28 X 1,5 cupric pipe cold water-Mineral wool 20 mm-20" 0.0015, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" ("ML-15 X 1,2 cupric pipe hot water-Mineral wool 20 mm-20" 0.001200000047683716, "Layer-Mineral wool 20 mm" 0.02) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          24 x IFCBUILDINGELEMENTPROXY | names: "Heater" | property sets: Pset_Draughting
          9 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32" 0.003200000047683716); layers "ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" ("ML-11/4" ( 42.4X3.2) steel pipe DN 32-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          20 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          5 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          2 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          1 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          4 x IFCENERGYCONVERSIONDEVICE | type IFCSPACEHEATERTYPE "H12016" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2061" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          19 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          6 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          6 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          54 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05); layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20 cold water" 0.002599999904632569) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          64 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "DI2557" | property sets: Pset_Draughting
          54 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" ("ML-3/4" ( 26.9X2.6) steel pipe DN 20-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2061" | property sets: Pset_Draughting
          8 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          61 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1/2" ( 21.3X2.6) steel pipe DN 15-Mineral wool 50 mm-50" ("ML-1/2" ( 21.3X2.6) steel pipe DN 15-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          46 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2060" | property sets: Pset_Draughting
          40 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" ("ML-1/2" ( 21.3X2.6) steel pipe DN 15 cold water-Mineral wool 50 mm-50" 0.002599999904632569, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          3 x IFCFLOWCONTROLLER | type IFCVALVETYPE "VA2063" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "TP2000" | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          12 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS0000" | material: layers "ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" ("ML-1" ( 33.7X3.2) steel pipe DN 25 cold water-Mineral wool 50 mm-50" 0.003200000047683716, "Layer-Mineral wool 50 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentPipeSegment
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_Draughting

Types
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103080K_1001" | RIGIDSEGMENT | 29 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "3" ( 88.9X4.0) steel pipe DN 80"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0800P_1002" | BEND | 25 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 80 3" Steel bend free angle"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0890P_1004" | BEND | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 80 3" Steel bend 90°"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS050101_000_X131103100K_1006" | RIGIDSEGMENT | 27 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "4" (114.3X4.5) steel pipe DN 100"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS1000P_1007" | BEND | 23 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 100 4" Steel bend free angle"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS1090P_1008" | BEND | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 100 4" Steel bend 90°"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002007K_1009" | RIGIDSEGMENT | 138 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "75MMX3.0M PP drain pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0007590P_1010" | BEND | 28 occurrences | property sets: Pset_PipeFittingTypeCommon | description "75 mm PP bend 90°"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010101_000_OPP0001107P_1013" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "Pipe reducer PP 110mm - 75mm"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002011K_1034" | RIGIDSEGMENT | 68 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "110MMX6,0M PP drain pipe"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0110075P_1017" | JUNCTION | 7 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110X 75 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001145P_1020" | BEND | 89 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110 mm PP bend 45°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0110110P_1019" | JUNCTION | 15 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110X 110 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0007500P_1018" | BEND | 11 occurrences | property sets: Pset_PipeFittingTypeCommon | description "75 mm PP bend free angle"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002011K_1014" | RIGIDSEGMENT | 152 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "110MMX3.0M PP drain pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001100P_1021" | BEND | 17 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110 mm PP bend free angle"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002016K_1023" | RIGIDSEGMENT | 24 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "160MMX6,0M PP drain pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001690P_1024" | BEND | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "160 mm PP bend 90°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001645P_1025" | BEND | 9 occurrences | property sets: Pset_PipeFittingTypeCommon | description "160 mm PP bend 45°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0160110P_1027" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "160X 110 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0160160P_1028" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "160X 160 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0160075P_1031" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "160X 75 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001600P_1029" | BEND | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "160 mm PP bend free angle"
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCWASTETERMINALTYPE "GU2104" | element type "GU010101_104_U111000011P_1033" | GULLYTRAP | 5 occurrences | property sets: Pset_WasteTerminalTypeGullyTrap | description "Floor gully 110mm square"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001190P_1035" | BEND | 38 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110 mm PP bend 90°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001130P_1036" | BEND | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110 mm PP bend 30°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0001160P_1042" | BEND | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "110 mm PP bend 60°"
  IFCSANITARYTERMINALTYPE "WC2152" | element type "WC030101_152_U231000001P_1047" | TOILETPAN | 11 occurrences | property sets: Pset_SanitaryTerminalTypeToiletPan | description "Water closet, pipe in pipe connection"
  IFCSANITARYTERMINALTYPE "WC2152" | element type "WC030101_152_WC-300903101943_1048" | TOILETPAN | 3 occurrences | property sets: Pset_SanitaryTerminalTypeToiletPan | description "Water closet, pipe in pipe connection 18cm"
  IFCSANITARYTERMINALTYPE "SI2152" | element type "SI010101_152_U211001001P_1049" | SINK | 6 occurrences | property sets: Pset_SanitaryTerminalTypeSink | description "Sink 56"
  IFCSANITARYTERMINALTYPE "SI2151" | element type "SI010101_151_U211000001P_1050" | SINK | 5 occurrences | property sets: Pset_SanitaryTerminalTypeSink | description "Sink 66"
  IFCWASTETERMINALTYPE "GU2101" | element type "GU010201_101_U111002007P_1051" | GULLYTRAP | 4 occurrences | property sets: Pset_WasteTerminalTypeGullyTrap | description "Floor gully 75mm circular"
  IFCSANITARYTERMINALTYPE "SI2900" | element type "SI030201_900_U313103001P_1052" | SINK | 1 occurrence | property sets: Pset_SanitaryTerminalTypeSink | description "Utility sink 500 x 400"
  IFCSANITARYTERMINALTYPE "SI2153" | element type "SI010101_153_U211002001P_1053" | SINK | 6 occurrences | property sets: Pset_SanitaryTerminalTypeSink | description "Sink 50"
  IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | element type "FH010101_060_FH-300903102501_1055" | HOSEREEL | 10 occurrences | property sets: Pset_FireSuppressionTerminalTypeHoseReel | description "Fire hose 825X225x140"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000054K_1057" | RIGIDSEGMENT | 11 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "54 X 2,0 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG5490P_1058" | BEND | 5 occurrences | property sets: Pset_PipeFittingTypeCommon | description "54MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB054028P_1072" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "54MM - 28 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB054035P_1066" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "54MM - 35 mm cupric t-part"
  IFCPIPESEGMENTTYPE "BD2000" | element type "BD000000_000_" | FLEXIBLESEGMENT | 1 occurrence
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010301_000_OKOBBH1042P_1104" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "54mm-42mm Reducer cupric"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000042K_1100" | RIGIDSEGMENT | 9 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "42 X 2,0 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB042028P_1106" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "42MM - 28 mm cupric t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG4290P_1110" | BEND | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "42MM 1/2 BEND 5040 M/1 muff cupric"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG4290P_1101" | BEND | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "42MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB042012P_1111" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "42MM - 12 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB042035P_1105" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "42MM - 35 mm cupric t-part"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010301_000_OKOBBH1035P_1123" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "42mm-35mm Reducer cupric"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000035K_1068" | RIGIDSEGMENT | 49 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "35 X 2,0 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG3590P_1069" | BEND | 33 occurrences | property sets: Pset_PipeFittingTypeCommon | description "35MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020201_000_X122000018K_1061" | RIGIDSEGMENT | 36 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "18 X 1,2 cupric pipe hot water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG1890P_1062" | BEND | 43 occurrences | property sets: Pset_PipeFittingTypeCommon | description "18MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB018015P_1067" | JUNCTION | 4 occurrences | property sets: Pset_PipeFittingTypeCommon | description "18MM - 15 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB018012P_1076" | JUNCTION | 10 occurrences | property sets: Pset_PipeFittingTypeCommon | description "18MM - 12 mm cupric t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG1890P_1063" | BEND | 6 occurrences | property sets: Pset_PipeFittingTypeCommon | description "18MM 1/2 BEND 5040 M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB035028P_1079" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "35MM - 28 mm cupric t-part"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010301_000_OKOBBH1028P_1083" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "35mm-28mm Reducer cupric"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000028K_1081" | RIGIDSEGMENT | 49 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "28 X 1,5 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB028015P_1086" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "28MM - 15 mm cupric t-part"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG2890P_1074" | BEND | 161 occurrences | property sets: Pset_PipeFittingTypeCommon | description "28MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020201_000_X122000015K_1070" | RIGIDSEGMENT | 23 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "15 X 1,2 cupric pipe hot water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG1590P_1071" | BEND | 41 occurrences | property sets: Pset_PipeFittingTypeCommon | description "15MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB015012P_1080" | JUNCTION | 11 occurrences | property sets: Pset_PipeFittingTypeCommon | description "15MM - 12 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020201_000_X122000012K_1077" | RIGIDSEGMENT | 42 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "12 X 1,0 cupric pipe hot water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG1290P_1078" | BEND | 103 occurrences | property sets: Pset_PipeFittingTypeCommon | description "12MM 1/1 BEND 5001 A M/1 muff cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB012015P_1097" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "12MM - 15 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB012012P_1090" | JUNCTION | 9 occurrences | property sets: Pset_PipeFittingTypeCommon | description "12MM - 12 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000015K_1087" | RIGIDSEGMENT | 37 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "15 X 1,2 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB015015P_1092" | JUNCTION | 19 occurrences | property sets: Pset_PipeFittingTypeCommon | description "15MM - 15 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020102_000_X121001015K_1091" | RIGIDSEGMENT | 150 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "15 X 2.5 mm wirsbo-pex pipe in pipes cold water"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020202_000_X122001015K_1096" | RIGIDSEGMENT | 24 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "15 X 2.5 mm wirsbo-pex pipe in pipes hot water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010103_000_BKOBBG1290P_1094" | BEND | 18 occurrences | property sets: Pset_PipeFittingTypeCommon | description "12MM BEND M/1 muff cupric free angle"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020202_000_X122001012K_1095" | RIGIDSEGMENT | 99 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "12 X 2.0 mm wirsbo-pex pipe in pipes hot water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB028012P_1107" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "28MM - 12 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000012K_1089" | RIGIDSEGMENT | 14 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "12 X 1,0 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010101_000_OPP0001105P_1115" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "Pipe reducer PP 110mm - 50mm"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002005K_1114" | RIGIDSEGMENT | 97 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "50MMX3,0M PP drain pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0005045P_1124" | BEND | 49 occurrences | property sets: Pset_PipeFittingTypeCommon | description "50 mm PP bend 45°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0005090P_1125" | BEND | 35 occurrences | property sets: Pset_PipeFittingTypeCommon | description "50 mm PP bend 90°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4110075P_1116" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "110X 75 mm X 45° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4110110P_1121" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "110X 110 mm X 45° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4110032P_1117" | JUNCTION | 5 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110X 32 mm X 45° PP t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS010101_000_X111002003K_1118" | RIGIDSEGMENT | 42 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "32MMX3,0M PP drain pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0003245P_1119" | BEND | 10 occurrences | property sets: Pset_PipeFittingTypeCommon | description "32 mm PP bend 45°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0003290P_1120" | BEND | 20 occurrences | property sets: Pset_PipeFittingTypeCommon | description "32 mm PP bend 90°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0007545P_1011" | BEND | 20 occurrences | property sets: Pset_PipeFittingTypeCommon | description "75 mm PP bend 45°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0110032P_1022" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "110X 32 mm X free° PP t-part"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010502_016_W531002130P_1160" | SECTIONALRADIATOR | 12 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK22K-412 1636W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010502_016_W531002130P_1161" | SECTIONALRADIATOR | 1 occurrence | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK22K-407 981W"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103032K_1162" | RIGIDSEGMENT | 93 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "11/4" ( 42.4X3.2) steel pipe DN 32"
  IFCVALVETYPE "VA2063" | element type "VA010101_063_X311000032K_1166" | AIRRELEASE | 8 occurrences | description "1 1/4" shut off valve, muff DN32"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0390P_1163" | BEND | 59 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 32 1 1/4" Steel bend 90°"
  IFCVALVETYPE "VA2060" | element type "VA020101_060_X323000032K_1168" | AIRRELEASE | 6 occurrences | description "1 1/4" throttle valve, muff DN32"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103040K_1170" | RIGIDSEGMENT | 11 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "11/2" ( 48.3X3.2) steel pipe DN 40"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST040020P_1175" | JUNCTION | 6 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/2"- 3/4" steel pipe t-part DN 40 -20"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0103P_1198" | TRANSITION | 4 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 40mm-32mm Reducer steel pipe"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0490P_1172" | BEND | 21 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 40 1 1/2" Steel bend 90°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST032015P_1248" | JUNCTION | 4 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/4"- 1/2" steel pipe t-part DN 32 -15"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0445P_1173" | BEND | 4 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 40 1 1/2" Steel bend 45°"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST032025P_1184" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/4"- 1" steel pipe t-part DN 32 -25"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0102P_1199" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 40mm-25mm Reducer steel pipe"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103025K_1222" | RIGIDSEGMENT | 47 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "1" ( 33.7X3.2) steel pipe DN 25"
  IFCVALVETYPE "VA2063" | element type "VA010101_063_X311000025K_1209" | AIRRELEASE | 7 occurrences | description "1" shut off valve, muff DN25"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST025020P_1192" | JUNCTION | 15 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1" - 3/4" steel pipe t-part DN 25 -20"
  IFCVALVETYPE "VA2060" | element type "VA020101_060_X323000025K_1212" | AIRRELEASE | 5 occurrences | description "1" throttle valve, muff DN25"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103020K_1176" | RIGIDSEGMENT | 102 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "3/4" ( 26.9X2.6) steel pipe DN 20"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0200P_1177" | BEND | 196 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 20 3/4 Steel bend free angle"
  IFCVALVETYPE "VA2060" | element type "VA020101_060_X323000020K_1210" | AIRRELEASE | 19 occurrences | description "3/4" throttle valve, muff DN20"
  IFCVALVETYPE "VA2063" | element type "VA010101_063_X311000020K_1207" | AIRRELEASE | 23 occurrences | description "3/4" shut off valve, muff DN20"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003020K_1178" | RIGIDSEGMENT | 239 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "3/4" ( 26.9X2.6) steel pipe DN 20 cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST020010P_1204" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "3/4" - 3/8" steel pipe t-part DN 20 -10"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST020015P_1179" | JUNCTION | 24 occurrences | property sets: Pset_PipeFittingTypeCommon | description "3/4" - 1/2" steel pipe t-part DN 20 -15"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST020020P_1201" | JUNCTION | 26 occurrences | property sets: Pset_PipeFittingTypeCommon | description "3/4" - 3/4" steel pipe t-part DN 20 -20"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003015K_1180" | RIGIDSEGMENT | 155 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "1/2" ( 21.3X2.6) steel pipe DN 15 cold water"
  IFCVALVETYPE "VA2063" | element type "VA010101_063_X311000015K_1206" | AIRRELEASE | 13 occurrences | description "1/2" shut off valve, muff DN15"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0190P_1181" | BEND | 88 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 15 1/2" Steel bend 90°"
  IFCVALVETYPE "VA2060" | element type "VA020101_060_X323000015K_1205" | AIRRELEASE | 12 occurrences | description "1/2" throttle valve, muff DN15"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003040K_1174" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "11/2" ( 48.3X3.2) steel pipe DN 40 cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST040032P_1182" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/2"-1 1/4" steel pipe t-part DN 40 -32"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003032K_1129" | RIGIDSEGMENT | 24 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "11/4" ( 42.4X3.2) steel pipe DN 32 cold water"
  IFCVALVETYPE "VA2063" | element type "VA010101_063_X311000040K_1208" | AIRRELEASE | 1 occurrence | description "1 1/2" shut off valve, muff DN40"
  IFCVALVETYPE "VA2060" | element type "VA020101_060_X323000040K_1211" | AIRRELEASE | 1 occurrence | description "1 1/2" throttle valve, muff DN40"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST032032P_1185" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/4"-1 1/4" steel pipe t-part DN 32 -32"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0102P_1189" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 32mm-25mm Reducer steel pipe"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST025015P_1193" | JUNCTION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1" - 1/2" steel pipe t-part DN 25 -15"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0102P_1191" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 25mm-20mm Reducer steel pipe"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003025K_1188" | RIGIDSEGMENT | 62 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "1" ( 33.7X3.2) steel pipe DN 25 cold water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0345P_1194" | BEND | 5 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 32 1 1/4" Steel bend 45°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0145P_1195" | BEND | 21 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 15 1/2" Steel bend 45°"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0290P_1200" | BEND | 42 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 25 1" Steel bend 90°"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0101P_1203" | TRANSITION | 10 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 20mm-15mm Reducer steel pipe"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS080101_000_X132103015K_1243" | RIGIDSEGMENT | 62 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "1/2" ( 21.3X2.6) steel pipe DN 15"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4075075P_1128" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "75 X 75 mm X 45° PP t-part"
  IFCFIRESUPPRESSIONTERMINALTYPE "FH2060" | element type "FH010101_060_FH-300903130623_1131" | HOSEREEL | 3 occurrences | property sets: Pset_FireSuppressionTerminalTypeHoseReel | description "Fire hose 700X225x140"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0003200P_1132" | BEND | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "32 mm PP bend free angle"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB035015P_1085" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "35MM - 15 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB035035P_1133" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "35MM - 35 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020102_000_X121001012K_1093" | RIGIDSEGMENT | 48 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "12 X 2.0 mm wirsbo-pex pipe in pipes cold water"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010101_000_BPP0003260P_1135" | BEND | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "32 mm PP bend 60°"
  IFCSANITARYTERMINALTYPE "SI2904" | element type "SI030101_904_U341102001P_1137" | SINK | 1 occurrence | property sets: Pset_SanitaryTerminalTypeSink | description "Kitchen sink cooking plate left"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB028028P_1130" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "28MM - 28 mm cupric t-part"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010301_000_OKOBBH1015P_1139" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "28mm-15mm Reducer cupric"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4110050P_1140" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "110X 50 mm X 45° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0075050P_1126" | JUNCTION | 13 occurrences | property sets: Pset_PipeFittingTypeCommon | description "75 X 50 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0075032P_1141" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "75 X 32 mm X free° PP t-part"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010402_016_W531002130P_1214" | SECTIONALRADIATOR | 1 occurrence | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK21K-407 756W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010403_016_W531002130P_1215" | SECTIONALRADIATOR | 28 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK21K-512 1518W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010403_016_W531002130P_1216" | SECTIONALRADIATOR | 7 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK21K-507 911W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010504_016_W531002130P_1217" | SECTIONALRADIATOR | 3 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK22K-630 5719W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010601_016_W531002130P_1239" | SECTIONALRADIATOR | 3 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK33K-330 4516W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010504_016_W531002130P_1218" | SECTIONALRADIATOR | 7 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK22K-612 2288W"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP000000_000_" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP000000_000_" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0245P_1220" | BEND | 6 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 25 1" Steel bend 45°"
  IFCVALVETYPE "VA2061" | element type "VA100107_061_065F212500_1233" | AIRRELEASE | 1 occurrence | description "Danfoss 2-way valve VS2 25, Kvs 4,00"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010102_000_BSTÅLS0230P_1221" | BEND | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 25 1" Steel bend 30°"
  IFCPIPEFITTINGTYPE "DI2557" | element type "DI020201_557_DI-021003153649_1223" | JUNCTION | 2 occurrences | description "Underfloor heating distributor"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST032020P_1224" | JUNCTION | 5 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1 1/4"- 3/4" steel pipe t-part DN 32 -20"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0102P_1227" | TRANSITION | 3 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 32mm-20mm Reducer steel pipe"
  IFCVALVETYPE "VA2061" | element type "VA100107_061_065F212000_1231" | AIRRELEASE | 2 occurrences | description "Danfoss 2-way valve VS2 20, Kvs 2,50"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0101P_1226" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 32mm-15mm Reducer steel pipe"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST015020P_1225" | JUNCTION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1/2" - 3/4" steel pipe t-part DN 15 -20"
  IFCVALVETYPE "VA2061" | element type "VA100107_061_065F211100_1228" | AIRRELEASE | 1 occurrence | description "Danfoss 2-way valve VS2 15, Kvs 0,25"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0110P_1235" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "DN 20mm-100mm Reducer steel pipe"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020103_000_X121003100K_1234" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_PipeSegmentTypeCommon | description "4" (114.3X4.5) steel pipe DN 100 cold water"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010201_000_OSTÅLR0102P_1202" | TRANSITION | 2 occurrences | property sets: Pset_PipeFittingTypeCommon | description "DN 20mm-20mm Reducer steel pipe"
  IFCSANITARYTERMINALTYPE "SI2902" | element type "SI030101_902_U341102001P_1142" | SINK | 1 occurrence | property sets: Pset_SanitaryTerminalTypeSink | description "Kitchen sink cooking plate right"
  IFCELECTRICAPPLIANCETYPE "WM2001" | element type "WM010101_001_U610001001P_1143" | WASHINGMACHINE | 1 occurrence | description "Washing machine connection right"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB035018P_1148" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "35MM - 18 mm cupric t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP4050050P_1147" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "50 X 50 mm X 45° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010301_000_THKB018018P_1153" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "18MM - 18 mm cupric t-part"
  IFCPIPESEGMENTTYPE "SS0000" | element type "SS020101_000_X121000018K_1099" | RIGIDSEGMENT | 6 occurrences | property sets: Pset_PipeSegmentTypeCommon | description "18 X 1,2 cupric pipe cold water"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0075075P_1127" | JUNCTION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "75 X 75 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010101_000_TPP0050050P_1152" | JUNCTION | 4 occurrences | property sets: Pset_PipeFittingTypeCommon | description "50 X 50 mm X free° PP t-part"
  IFCPIPEFITTINGTYPE "CH2000" | element type "CH010101_000_OPP0000705P_1154" | TRANSITION | 1 occurrence | property sets: Pset_PipeFittingTypeCommon | description "Pipe reducer PP 75mm - 50mm"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010403_016_W531002130P_1240" | SECTIONALRADIATOR | 1 occurrence | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK21K-516 2024W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010601_016_W531002130P_1241" | SECTIONALRADIATOR | 2 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK33K-322 3312W"
  IFCSPACEHEATERTYPE "H12016" | element type "H1010201_016_W531002130P_1242" | SECTIONALRADIATOR | 4 occurrences | property sets: Pset_SpaceHeaterTypeCommon | description "TIPRO NOVA KOMPAKT TK11-328 1594W"
  IFCVALVETYPE "VA2061" | element type "VA100107_061_065F211300_1246" | AIRRELEASE | 1 occurrence | description "Danfoss 2-way valve VS2 15, Kvs 0,63"
  IFCPIPEFITTINGTYPE "TP2000" | element type "TP010201_000_TSST015015P_1244" | JUNCTION | 5 occurrences | property sets: Pset_PipeFittingTypeCommon | description "1/2" - 1/2" steel pipe t-part DN 15 -15"

Property sets
  Storey quantities | quantities | on 6 objects (6 IFCBUILDINGSTOREY)
    TotalHeight = 2.75 [METRE]
  Storey quantities | quantities | on 2 objects (2 IFCBUILDINGSTOREY)
    TotalHeight = 0. [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 31 objects (31 IFCFLOWSEGMENT)
    Length = 0.1200012043118477 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 28 objects (28 IFCFLOWSEGMENT)
    Length = 0.1150016784667969 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 26 objects (26 IFCFLOWSEGMENT)
    Length = 0.1150024384260178 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 17 objects (17 IFCFLOWSEGMENT)
    Length = 3.794997453689575 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Length = 3.794998168945313 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 11 objects (11 IFCFLOWSEGMENT)
    Length = 2.650000095367432 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 9 objects (9 IFCFLOWSEGMENT)
    Length = 2.109999895095825 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 9 objects (9 IFCFLOWSEGMENT)
    Length = 2.210000276565552 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment: 1698 more contents on 2073 objects not shown
  Pset_Draughting | properties | on 723 objects (425 IFCFLOWSEGMENT, 298 IFCFLOWFITTING)
    Colour: Red = 210 (IFCINTEGER); Green = 210 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0321 LEDNING VARME" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 721 objects (403 IFCFLOWSEGMENT, 318 IFCFLOWFITTING)
    Colour: Red = 64 (IFCINTEGER); Green = 230 (IFCINTEGER); Blue = 230 (IFCINTEGER)
    LayerName = "0321 LEDNING VARME" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 703 objects (380 IFCFLOWSEGMENT, 323 IFCFLOWFITTING)
    Colour: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 255 (IFCINTEGER)
    LayerName = "0312 LEDNING SANITÆR" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 430 objects (248 IFCFLOWSEGMENT, 182 IFCFLOWFITTING)
    Colour: Red = 0 (IFCINTEGER); Green = 240 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0312 LEDNING SANITÆR" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 395 objects (216 IFCFLOWSEGMENT, 179 IFCFLOWFITTING)
    Colour: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 255 (IFCINTEGER)
    LayerName = "0311 LEDNING GRUNN" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 382 objects (207 IFCFLOWSEGMENT, 175 IFCFLOWFITTING)
    Colour: Red = 255 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0312 LEDNING SANITÆR" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 100 objects (100 IFCFLOWCONTROLLER)
    Colour: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0321 LEDNING VARME" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 69 objects (69 IFCENERGYCONVERSIONDEVICE)
    Colour: Red = 64 (IFCINTEGER); Green = 230 (IFCINTEGER); Blue = 230 (IFCINTEGER)
    LayerName = "UTSTYR VARME" (IFCIDENTIFIER)
  Pset_Draughting: 9 more contents on 194 objects not shown
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.1053000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.1143000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.1053000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.11] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.1143000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.01560000038146973] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.018] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.018] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.01260000038146973] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.01] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.012] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.012] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.02] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.012] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.012] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.016] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.036] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.04240000152587891] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon: 13 more contents on 0 objects not shown
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.1053000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.11] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.1143000030517578] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "OTHER" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.025, 0.025, 0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.11, 0.11, 0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.028, 0.028, 0.028] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "JUNCTION_TEE_Y" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.03600000143051148] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.04240000152587891] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "BEND_90DEGREE" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.03600000143051148] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.04240000152587891] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "BEND_45DEGREE" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.03600000143051148, 0.02729999923706055] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032, 0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.04240000152587891, 0.03370000076293946] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.02170000171661377, 0.02170000076293945, 0.02170000076293945] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.02, 0.02, 0.02] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.02690000152587891, 0.02690000152587891, 0.02690000152587891] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "JUNCTION_TEE_SQUARE" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.02170000171661377, 0.01610000038146973] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.02, 0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.02690000152587891, 0.02129999923706055] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeFittingTypeCommon | properties | on 2 type objects
    InnerDiameter = [0.03600000143051148, 0.01260000038146973, 0.02729999923706055] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032, 0.032, 0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.04240000152587891, 0.015, 0.03370000076293946] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "JUNCTION_TEE_Y" (IFCLABEL)
  Pset_PipeFittingTypeCommon: 91 more contents on 0 objects not shown
  Pset_WasteTerminalTypeGullyTrap | properties | on 1 type object
    GullyType in {"Unset"} (IFCTEXT)
    NominalBodyDepth = 0.11 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalBodyLength = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalBodyWidth = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    OutletConnectionSize = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_WasteTerminalTypeGullyTrap | properties | on 1 type object
    GullyType in {"Unset"} (IFCTEXT)
    NominalBodyDepth = 0.075 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalBodyLength = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalBodyWidth = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    OutletConnectionSize = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_SanitaryTerminalTypeToiletPan | properties | on 1 type object
    NominalDepth = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 0.65 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalWidth = 0.4 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ToiletType in {"CloseCoupled"} (IFCTEXT)
  Pset_SanitaryTerminalTypeToiletPan | properties | on 1 type object
    NominalDepth = 0.226 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 0.018 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalWidth = 0.4 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ToiletType in {"CloseCoupled"} (IFCTEXT)
  Pset_SanitaryTerminalTypeSink | properties | on 4 type objects
    DrainSize = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDepth = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 0.65 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalWidth = 0.52 (IFCPOSITIVELENGTHMEASURE) [METRE]
    SinkType in {"Unset"} (IFCTEXT)
  Pset_SanitaryTerminalTypeSink | properties | on 1 type object
    DrainSize = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDepth = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 0.63 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalWidth = 0.51 (IFCPOSITIVELENGTHMEASURE) [METRE]
    SinkType in {"Unset"} (IFCTEXT)
  Pset_SanitaryTerminalTypeSink | properties | on 1 type object
    DrainSize = 0.05 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDepth = 0. (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalLength = 0.6 (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalWidth = 0.49 (IFCPOSITIVELENGTHMEASURE) [METRE]
    SinkType in {"Unset"} (IFCTEXT)
  Pset_FireSuppressionTerminalTypeHoseReel | properties | on 2 type objects
    HoseReelType in {"Reel"} (IFCTEXT)
    InletConnectionSize = 50. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 1636. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 981. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 756. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 1518. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 911. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 5719. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 4516. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon | properties | on 1 type object
    HeatingSource in {"HOTWATER"} (IFCTEXT)
    OutputCapacity = 2288. (IFCPOWERMEASURE) [WATT]
    TemperatureClassification in {"LOWTEMPERATURE"} (IFCTEXT)
  Pset_SpaceHeaterTypeCommon: 3 more contents on 0 objects not shown