IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Barcelona_Pavillon.ifc"
Time stamp: "2013-03-01T11:21:05"
Preprocessor: "Autodesk Revit 2013"
Originating system: "20120221_2030(x64)"
Application: "Autodesk Revit 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013"

People and organizations
  Person "morten" "jensen" of Organization (no name given)
  Owner history of Person "morten" "jensen" of Organization (no name given) | application "Autodesk Revit 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level -0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 7 elements
          5 x IFCWALLSTANDARDCASE | object type "Basic Wall:Generic - 200mm:398" | names: "Basic Wall:Generic - 200mm:178900", "Basic Wall:Generic - 200mm:179008", "Basic Wall:Generic - 200mm:179733" (+2 more) | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Constraints, Dimensions, Phasing, Structural, Pset_WallCommon, Identity Data
          1 x IFCSLAB | object type "Floor:Generic 1350mm" | FLOOR | names: "Floor:Generic 1350mm:186263" | material: layers "Floor:Generic 1350mm" ("Default Floor" 1350.) | property sets: Phasing, Dimensions, Structural, Constraints, Pset_SlabCommon, Graphics
          1 x IFCSTAIR | object type "Stair:190mm max riser 250mm going:28598" | names: "Stair:190mm max riser 250mm going:187003" | parts: 1 IFCSTAIR | property sets: Graphics, Phasing, Dimensions, Constraints, Structural, Pset_StairCommon
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 1500.
        contains 21 elements
          1 x IFCSLAB | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:177074" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Phasing, Constraints, Dimensions, Structural, Pset_SlabCommon, Construction
          5 x IFCWALLSTANDARDCASE | object type "Basic Wall:Generic - 200mm:398" | names: "Basic Wall:Generic - 200mm:178739", "Basic Wall:Generic - 200mm:179069", "Basic Wall:Generic - 200mm:179647" (+2 more) | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Constraints, Phasing, Structural, Dimensions, Pset_WallCommon, Identity Data
          4 x IFCWALLSTANDARDCASE | object type "Basic Wall:Generic - 50mm:180254" | names: "Basic Wall:Generic - 50mm:180420", "Basic Wall:Generic - 50mm:180524", "Basic Wall:Generic - 50mm:180656" (+1 more) | material: layers "Basic Wall:Generic - 50mm" ("Default Wall" 50.) | property sets: Phasing, Structural, Constraints, Dimensions, Pset_WallCommon, Identity Data
          7 x IFCCURTAINWALL | object type "Curtain Wall:Curtain Wall:334" | names: "Curtain Wall:Curtain Wall:183068", "Curtain Wall:Curtain Wall:183263", "Curtain Wall:Curtain Wall:183946" (+4 more) | parts: 100 IFCMEMBER, 31 IFCPLATE | property sets: Pset_CurtainWallCommon, Vertical Grid Pattern, Phasing, Constraints, Horizontal Grid Pattern, Dimensions
          4 x IFCCURTAINWALL | object type "Curtain Wall:Curtain Wall Zero Grid lines:185560" | names: "Curtain Wall:Curtain Wall Zero Grid lines:185787", "Curtain Wall:Curtain Wall Zero Grid lines:185949", "Curtain Wall:Curtain Wall Zero Grid lines:186001" (+1 more) | parts: 16 IFCMEMBER, 4 IFCPLATE | property sets: Pset_CurtainWallCommon, Horizontal Grid Pattern, Constraints, Structural, Vertical Grid Pattern, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | elevation 4500.
        contains 2 elements
          2 x IFCROOF | object type "Basic Roof:Generic - 125mm" | names: "Basic Roof:Generic - 125mm:187494", "Basic Roof:Generic - 125mm:187551" | parts: 2 IFCSLAB | property sets: Construction, Dimensions, Constraints, Phasing, Pset_RoofCommon, Identity Data

Property sets
  Phasing | properties | on 188 objects (116 IFCMEMBER, 35 IFCPLATE, 14 IFCWALLSTANDARDCASE, 11 IFCCURTAINWALL)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints | properties | on 116 objects (116 IFCMEMBER)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 35 objects (35 IFCPLATE)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 11 objects (11 IFCCURTAINWALL)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 2 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (3 IFCWALLSTANDARDCASE, 2 IFCOPENINGELEMENT)
    Base Constraint = "Level: Level 0" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 2 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4500. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 5 objects (2 IFCROOF, 2 IFCSLAB, 1 IFCOPENINGELEMENT)
    Base Level = "Level: Level 2" (IFCLABEL)
    Base Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cutoff Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 4 objects (2 IFCOPENINGELEMENT, 2 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 0" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 0 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Constraint = "Level: Level 2" (IFCLABEL)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 4500. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Constraints: 7 more contents on 8 objects not shown
  Dimensions | properties | on 116 objects (116 IFCMEMBER)
    Width on side 1 = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Width on side 2 = 15. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 46 objects (46 IFCMEMBER)
    Length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 35 objects (35 IFCPLATE)
    Thickness = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 10 objects (10 IFCPLATE)
    Area = 2856210. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Height = 2940. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 971.5 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 10 objects (10 IFCMEMBER)
    Length = 971.5 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 10 objects (10 IFCMEMBER)
    Length = 971.500000000003 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 8 objects (8 IFCPLATE)
    Area = 2612925. (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Height = 2940. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 888.749999999999 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 8 objects (8 IFCMEMBER)
    Length = 888.750000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions: 49 more contents on 99 objects not shown
  Structural | properties | on 29 objects (14 IFCWALLSTANDARDCASE, 11 IFCCURTAINWALL, 4 IFCOPENINGELEMENT)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = 0 (IFCINTEGER)
  Structural | properties | on 2 objects (2 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 1 object (1 IFCSTAIR)
    Rebar Cover = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic - 125mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic 150mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic 1350mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 10 objects (10 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 50mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 7 objects (7 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall:Curtain Wall" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Curtain Wall:Curtain Wall Zero Grid lines" (IFCIDENTIFIER)
  Vertical Grid Pattern | properties | on 7 objects (7 IFCCURTAINWALL)
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = 2 (IFCINTEGER)
    Spacing = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 4 objects (4 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 4 objects (4 IFCCURTAINWALL)
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = 0 (IFCINTEGER)
    Spacing = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 3 objects (3 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 1 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 3 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 9 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 7 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vertical Grid Pattern | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 4 (IFCINTEGER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid Pattern | properties | on 11 objects (11 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = 1 (IFCINTEGER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Horizontal Grid Pattern | properties | on 11 objects (11 IFCCURTAINWALL)
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = 0 (IFCINTEGER)
    Spacing = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 25 objects (14 IFCWALLSTANDARDCASE, 5 IFCOPENINGELEMENT, 4 IFCSLAB, 2 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCSTAIR)
    Down arrow = TRUE (IFCBOOLEAN)
    Down label = TRUE (IFCBOOLEAN)
    Down text = "DN" (IFCLABEL)
    Show Up arrow in all views = FALSE (IFCBOOLEAN)
    Up arrow = TRUE (IFCBOOLEAN)
    Up label = TRUE (IFCBOOLEAN)
    Up text = "UP" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCSTAIR)
    Break Symbol in Plan = TRUE (IFCBOOLEAN)
    Text Font = "Arial" (IFCLABEL)
    Text Size = 0.00820209973753281 (IFCREAL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 8 (IFCINTEGER)
    NumberOfTreads = 7 (IFCINTEGER)
    Reference = "190mm max riser 250mm going" (IFCIDENTIFIER)
    RiserHeight = 187.5 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    TreadLength = 250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 116 objects (116 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "-3" (IFCLABEL)
    Thickness = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 14 objects (10 IFCWALLSTANDARDCASE, 4 IFCOPENINGELEMENT)
    Function = 1 (IFCINTEGER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  Construction | properties | on 11 objects (11 IFCCURTAINWALL)
    Automatically Embed = FALSE (IFCBOOLEAN)
    Function = 1 (IFCINTEGER)
    Join Condition = 0 (IFCINTEGER)
  Construction | properties | on 5 objects (2 IFCROOF, 2 IFCSLAB, 1 IFCOPENINGELEMENT)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Maximum Ridge Height = 4625. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = 33615 (IFCINTEGER)
  Construction | properties | on 5 objects (2 IFCROOF, 2 IFCSLAB, 1 IFCOPENINGELEMENT)
    Default Thickness = 125. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    Function = 1 (IFCINTEGER)
    Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 1350. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = 0 (IFCINTEGER)
  Construction: 1 more content on 1 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 306611726.286192 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Reference = "Generic - 125mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 89870400.0002312 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Reference = "Generic - 125mm" (IFCIDENTIFIER)
  Identity Data | properties | on 151 objects (116 IFCMEMBER, 35 IFCPLATE)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
  Identity Data | properties | on 37 objects (14 IFCWALLSTANDARDCASE, 11 IFCCURTAINWALL, 5 IFCOPENINGELEMENT, 4 IFCSLAB)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCLABEL)
    Building Name = "" (IFCLABEL)
    Organization Description = "" (IFCLABEL)
    Organization Name = "" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 3 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCLABEL)
    Project Address = "Enter address here" (IFCLABEL)
    Project Issue Date = "Issue Date" (IFCLABEL)
    Project Name = "Project Name" (IFCLABEL)
    Project Number = "Project Number" (IFCLABEL)
    Project Status = "Project Status" (IFCLABEL)
  Analytical Properties | properties | on 35 objects (35 IFCPLATE)
    Analytic Construction = "1/8 in Pilkington single glazing" (IFCLABEL)
    Construction Type Id = "GSP4R" (IFCLABEL)
    Heat Transfer Coefficient (U) = 6.7069 (IFCREAL)
    Solar Heat Gain Coefficient = 0.86 (IFCREAL)
    Thermal Resistance (R) = 0.149100180411218 (IFCREAL)
    Visual Light Transmittance = 0.9 (IFCREAL)
  Analytical Properties | properties | on 25 objects (14 IFCWALLSTANDARDCASE, 5 IFCOPENINGELEMENT, 4 IFCSLAB, 2 IFCROOF)
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 116 objects (116 IFCMEMBER)
    Material = "Aluminium" (IFCLABEL)
  Materials and Finishes | properties | on 35 objects (35 IFCPLATE)
    Material = "Glass" (IFCLABEL)
  Treads | properties | on 1 object (1 IFCSTAIR)
    Apply Nosing Profile = 0 (IFCINTEGER)
    Minimum Tread Depth = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Nosing Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
  Stringers | properties | on 1 object (1 IFCSTAIR)
    Landing Carriage Height = 303.27081688339 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Stringer = 1 (IFCINTEGER)
    Middle Stringers = 0 (IFCINTEGER)
    Open Stringer Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Stringer = 1 (IFCINTEGER)
    Stringer Carriage Height = 152. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Height = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Stringer Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Stringers at Top = 0 (IFCINTEGER)
  Risers | properties | on 1 object (1 IFCSTAIR)
    Begin with Riser = TRUE (IFCBOOLEAN)
    End with Riser = TRUE (IFCBOOLEAN)
    Maximum Riser Height = 190. (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Thickness = 12.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Type = 1 (IFCINTEGER)
    Riser to Tread Connection = 0 (IFCINTEGER)