IFC building model
Schema: "IFC2X2_FINAL"
Description: "IFC2X2_FINAL"
File name: "HiB_DuctWork.ifc"
Time stamp: "2005-04-01T13:16:04"
Author: "ST"
Organization: "Data Design System ASA"
Preprocessor: "DDS-IFC v1.0"
Originating system: "Building Services Partner Version 6.35 Prerel build 1/4-2005"
Authorization: "DDS"
Application: "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS"
Application: "Common Building functions Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Common Building functions" by Organization "DDS"
Application: "DuctWork Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "DuctWork" by Organization "DDS"

People and organizations
  3 x Person "Stian" "Tonheim" of Organization "DDS"
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "Building Services Partner Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "Building Services Partner" by Organization "DDS" | change NOCHANGE | created 1112354164 (2005-04-01T11:16:04Z)
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "DuctWork Version 6.35 Prerel build 1/4-2005" version "Version 6.35 Prerel build 1/4-2005" identifier "DuctWork" by Organization "DDS" | change NOCHANGE | created 1112354102 (2005-04-01T11:15:02Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  MASSUNIT: GRAM
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICRESISTANCEUNIT: OHM
  POWERUNIT: WATT
  MASSUNIT: GRAM
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  PRESSUREUNIT: PASCAL
  LUMINOUSFLUXUNIT: LUMEN
  ILLUMINANCEUNIT: LUX
  VOLUMEUNIT: CUBIC_METRE
  TIMEUNIT: SECOND
  VOLUMETRICFLOWRATEUNIT: derived

Spatial structure
IFCPROJECT "DDS Project"
  IFCSITE | postal address: "Bergen"
    IFCBUILDING | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "Ventilation in ground" | COMPLEX | elevation 0. | description "Ventilation in ground"
        contains 709 elements
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_FlowSegmentDuctSegment, Pset_Draughting
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | property sets: Pset_Draughting
          462 x IFCDISTRIBUTIONPORT
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          78 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim" ("Layer-Rectangular duct zinc plated free dim" 0.028) | property sets: Pset_FlowSegmentDuctSegment, Pset_Draughting
          10 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          10 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated 500x400" ("Layer-Rectangular duct zinc plated 500x400" 0.028); layers "ML-Rectangular duct zinc plated 500x400-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 500x400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          67 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          20 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 630 mm" ("Layer-Circular duct zinc plated 630 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
      IFCBUILDINGSTOREY "Ventilation basement" | COMPLEX | elevation 0. | description "Ventilation basement"
        contains 2296 elements
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-400x300-Insulation fire 30 mm-50" ("Layer-400x300" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1498 x IFCDISTRIBUTIONPORT
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-1200 x 400-Insulation fire 30 mm-50" ("Layer-1200 x 400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-400x700-Insulation fire 30 mm-50" ("Layer-400x700" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-500x600-Insulation fire 30 mm-50" ("Layer-500x600" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          30 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "2.1.2", "2.1.4", "2.1.5" (+10 more) | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028); layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          28 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "2.1.4", "2.1.6", "3.2.7" (+18 more) | property sets: Pset_Draughting
          15 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "2.1.2", "3.2.5", "3.5.4" (+9 more) | property sets: Pset_Draughting
          8 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "2.1.0", "3.1.11", "3.2.3" (+1 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.4.5", "8.6.2" | material: layers "ML-Rectangular duct zinc plated 600x500-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 600x500" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Rectangular duct zinc plated 600x500" ("Layer-Rectangular duct zinc plated 600x500" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | property sets: Pset_Draughting
          12 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          35 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "1.1.5", "3.1.0", "3.1.2" (+21 more) | property sets: Pset_Draughting
          6 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "1.1.3", "3.1.13", "1.32.2" (+2 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          25 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.15.1", "4.15.3", "4.15.5" (+13 more) | material: layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "4.15.6", "7.4.6" | property sets: Pset_Draughting
          33 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "1.36.0", "1.35.0", "1.24.0" (+23 more) | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "8.40.9" | property sets: Pset_Draughting
          16 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.8.2", "4.8.4", "4.8.5" (+5 more) | material: layers "ML-Circular duct zinc plated 125 mm" ("Layer-Circular duct zinc plated 125 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "4.10.0", "4.9.0" | property sets: Pset_FlowTerminalAirTerminal, Pset_Draughting
          7 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "8.42.0", "8.41.0" | property sets: Pset_Draughting
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "8.40.14", "8.42.4", "8.41.4" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "2.1.8", "2.1.10", "3.2.9" (+2 more) | property sets: Pset_Draughting
          15 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "2.1.11", "3.2.12", "1.37.3" (+12 more) | property sets: Pset_Draughting
          12 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "2.3.1", "2.2.1", "3.3.1" (+4 more) | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028); layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "2.2.0", "3.3.0", "3.4.0" (+1 more) | property sets: Pset_FlowTerminalAirTerminal, Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-1300x400" ("Layer-1300x400" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "3.2.0" | property sets: Pset_Draughting
          2 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2002" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "1.1.2", "9.1.1", "9.1.3" (+2 more) | material: layers "ML-1300x500" ("Layer-1300x500" 0.028); layers "ML-1300x500-Insulation fire 30 mm-50" ("Layer-1300x500" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "1.1.0" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "1.1.5", "1.1.6", "1.1.9" (+5 more) | material: layers "ML-Rectangular duct zinc plated 1200x500" ("Layer-Rectangular duct zinc plated 1200x500" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "1.1.7", "1.2.2", "1.3.0" (+1 more) | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "1.2.0", "1.32.4", "1.21.0" (+6 more) | property sets: Pset_Draughting
          16 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "1.5.0", "1.34.0", "1.23.0" (+8 more) | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "3.1.1", "3.1.3" | material: layers "ML-Rectangular duct zinc plated 500x400-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 500x400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "3.1.5", "3.1.7", "3.1.10" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "3.1.4", "3.1.6" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "3.1.8" | property sets: Pset_Draughting
          5 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "3.1.13", "3.1.15", "3.1.16" (+2 more) | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "3.1.17", "1.32.6", "1.33.0" (+4 more) | property sets: Pset_Draughting
          4 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "3.5.2", "1.32.0", "1.14.0" (+1 more) | property sets: Pset_Draughting
          24 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "1.32.2", "1.32.4", "1.32.6" (+21 more) | material: layers "ML-Rectangular duct zinc plated 400x300" ("Layer-Rectangular duct zinc plated 400x300" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          16 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "1.37.2", "1.37.5", "1.29.2" (+13 more) | material: layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          16 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "1.37.0", "1.37.2", "1.29.4" (+13 more) | property sets: Pset_Draughting
          23 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "1.39.1", "1.38.1", "1.36.1" (+20 more) | material: layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          18 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "1.38.0", "1.36.2", "1.35.2" (+14 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          6 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "1.29.0", "4.13.0", "4.7.0" (+3 more) | property sets: Pset_Draughting
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "1.21.2", "1.21.4", "9.1.0" (+1 more) | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "1.25.0", "1.25.2", "6.2.0" | property sets: Pset_Draughting
          12 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "1.14.4", "1.14.6", "1.6.4" (+9 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "1.6.10", "4.5.0" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.1.2", "7.1.2", "7.2.2" (+1 more) | material: layers "ML-1600x1000" ("Layer-1600x1000" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "4.1.0" | property sets: Pset_Draughting
          14 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.1.5", "4.2.1", "4.2.3" (+11 more) | material: layers "ML-Rectangular duct zinc plated 1200x400" ("Layer-Rectangular duct zinc plated 1200x400" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "4.1.3", "7.2.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "4.3.10" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "4.4.0" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.13.2", "4.13.3", "4.13.6" (+1 more) | material: layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.11.1", "4.11.3", "4.11.6" (+1 more) | material: layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "4.11.4", "4.8.6", "4.8.8" (+2 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "4.11.6" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.11.10", "4.11.12", "4.12.1" (+8 more) | material: layers "ML-Circular duct zinc plated 100 mm" ("Layer-Circular duct zinc plated 100 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "4.12.0" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "4.8.0" | property sets: Pset_Draughting
          1 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "4.8.2" | property sets: Pset_Draughting
          16 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "4.7.2", "4.7.4", "4.7.5" (+13 more) | material: layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          16 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.1.2", "8.2.1", "8.2.4" (+10 more) | material: layers "ML-Rectangular duct zinc plated 1000x500" ("Layer-Rectangular duct zinc plated 1000x500" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "8.1.0", "8.2.2" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "8.3.12" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "8.4.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | names: "8.5.0" | property sets: Pset_Draughting
          12 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.54.4", "8.54.6", "8.54.7" (+9 more) | material: layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "8.54.2", "8.51.0" | property sets: Pset_Draughting
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "8.54.12", "8.54.14", "8.51.6" (+5 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "8.54.15" | property sets: Pset_Draughting
          9 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.55.1", "8.56.1", "8.52.1" (+6 more) | material: layers "ML-Circular duct zinc plated 200 mm" ("Layer-Circular duct zinc plated 200 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          8 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2301" | names: "8.56.0", "8.52.0", "8.53.0" (+4 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "8.51.9" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.43.2", "8.43.4", "8.43.6" | material: layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "8.40.2" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "8.7.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "8.19.4" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 630 mm" ("Layer-Circular duct zinc plated 630 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "2.1.0", "6.1.10", "6.1.14" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2801" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "4.14.12" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.45.2", "8.45.5", "8.48.2" (+1 more) | material: layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.46.1", "8.49.1", "8.47.1" (+1 more) | material: layers "ML-Circular duct zinc plated 200 mm" ("Layer-Circular duct zinc plated 200 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          7 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.1.1", "5.1.4", "5.2.4" (+4 more) | material: layers "ML-1600x400-Insulation fire 30 mm-50" ("Layer-1600x400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "5.1.2" | property sets: Pset_Draughting
          1 x IFCENERGYCONVERSIONDEVICE | type IFCAIRTOAIRHEATRECOVERYTYPE "DH2001" | names: "5.2.2" | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2012" | names: "5.2.4" | property sets: Pset_Draughting
          2 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "5.2.6" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "5.2.10" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.49.2", "5.51.2" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | names: "5.49.0" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "5.50.0", "9.1.4" | property sets: Pset_Draughting
          14 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.70.1", "2.1.2", "2.1.4" (+6 more) | material: layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "5.70.0" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.52.1" | material: layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "5.52.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWMOVINGDEVICE | type IFCFANTYPE "GF2500" | property sets: Pset_Draughting
          1 x IFCFLOWMOVINGDEVICE | type IFCFANTYPE "GF2500" | property sets: Pset_Draughting
          1 x IFCFLOWMOVINGDEVICE | type IFCFANTYPE "GF2500" | property sets: Pset_Draughting
          4 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "2.2.8", "4.15.8", "7.4.8" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "2.1.2" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "2.2.2", "2.2.4" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "2.2.10" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-2600x1600" ("Layer-2600x1600" 0.028); layers "ML-2600x1600-Insulation fire 30 mm-50" ("Layer-2600x1600" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim" ("Layer-Rectangular duct zinc plated free dim" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-1700x600-Insulation fire 30 mm-50" ("Layer-1700x600" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | property sets: Pset_Draughting
          5 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.1.1", "5.1.3", "5.1.5" (+1 more) | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Rectangular duct zinc plated free dim" ("Layer-Rectangular duct zinc plated free dim" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "5.1.6"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "7.1.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "7.5.4"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "4.15.14" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "7.4.14" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.1.1", "6.1.3", "6.1.5" (+5 more) | material: layers "ML-Rectangular duct zinc plated 1000x600" ("Layer-Rectangular duct zinc plated 1000x600" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.2.1", "6.2.3", "6.27.1" | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "6.2.4" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.5.1", "6.5.3" | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "6.5.2" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "6.27.2" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-2000x1500-Insulation fire 30 mm-50" ("Layer-2000x1500" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "9.2.0" | property sets: Pset_Draughting
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "9.4.1", "9.5.1" | material: layers "ML-Circular duct zinc plated 630 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 630 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "9.4.0"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "9.5.0"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
      IFCBUILDINGSTOREY "Ventilation 1th floor" | COMPLEX | elevation 2.75 | description "Ventilation 1th floor"
        contains 3982 elements
          10 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-400x300-Insulation fire 30 mm-50" ("Layer-400x300" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2652 x IFCDISTRIBUTIONPORT
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-1200 x 400-Insulation fire 30 mm-50" ("Layer-1200 x 400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-500x600-Insulation fire 30 mm-50" ("Layer-500x600" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          14 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "5.6.0", "5.6.2", "5.36.0" (+2 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | property sets: Pset_Draughting
          34 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.19.2", "5.19.4", "5.19.6" (+18 more) | material: layers "ML-Rectangular duct zinc plated 500x400-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 500x400" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Rectangular duct zinc plated 500x400" ("Layer-Rectangular duct zinc plated 500x400" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          18 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "5.19.4", "5.20.0", "5.7.0" (+2 more) | property sets: Pset_Draughting
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "IT2099" | names: "8.7.8", "6.2.10" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          9 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "5.19.0", "5.6.4", "5.36.4" (+3 more) | property sets: Pset_Draughting
          8 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "5.19.2", "5.6.6", "5.36.6" | property sets: Pset_Draughting
          3 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          30 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.29.2", "5.29.5", "5.22.2" (+24 more) | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028); layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          13 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "8.7.2", "5.52.2", "6.5.2" | property sets: Pset_Draughting
          35 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "8.18.6", "8.15.6", "8.14.6" (+12 more) | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-400x700-Insulation fire 30 mm-50" ("Layer-400x700" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated 600x300-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 600x300" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          32 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 315 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 315 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          3 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | property sets: Pset_Draughting
          62 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "5.44.0", "5.44.2", "5.41.0" (+25 more) | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "5.52.8", "5.60.4", "6.13.4" | property sets: Pset_Draughting
          43 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.52.13", "5.52.15", "5.53.2" (+20 more) | material: layers "ML-Circular duct zinc plated 250 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 250 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          64 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "8.7.0", "8.7.9", "8.7.31" (+40 more) | property sets: Pset_Draughting
          17 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "5.52.6", "5.54.4", "5.55.2" (+6 more) | property sets: Pset_Draughting
          39 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "5.44.3", "5.41.3", "5.11.3" (+19 more) | property sets: Pset_Draughting
          44 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.67.2", "5.67.4", "5.67.6" (+28 more) | material: layers "ML-Circular duct zinc plated 200 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 200 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 200 mm" ("Layer-Circular duct zinc plated 200 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          20 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "8.7.13", "5.67.4", "5.67.6" (+11 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          51 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.16.1", "8.16.3", "8.16.6" (+36 more) | material: layers "ML-Circular duct zinc plated 160 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 160 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          13 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "5.68.0", "5.69.0", "5.66.4" (+4 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          42 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.7.1", "8.7.4", "8.7.5" (+14 more) | material: layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          15 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "5.29.0", "5.29.2", "5.22.0" (+8 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          19 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.60.2", "5.60.4", "5.60.6" (+3 more) | material: layers "ML-Circular duct zinc plated 315 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 315 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          62 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "5.48.2", "5.47.2", "5.45.0" (+26 more) | property sets: Pset_Draughting
          21 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "8.7.11", "8.7.15", "8.7.17" (+7 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "8.16.6" | property sets: Pset_Draughting
          108 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.18.1", "8.18.3", "8.18.6" (+54 more) | material: layers "ML-Circular duct zinc plated 125 mm" ("Layer-Circular duct zinc plated 125 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          14 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "8.18.10", "8.15.10", "8.14.10" (+8 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          5 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          35 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated 400x300-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 400x300" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Rectangular duct zinc plated 400x300" ("Layer-Rectangular duct zinc plated 400x300" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          32 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 250 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 250 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          13 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          28 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "5.48.0", "5.47.0", "5.18.0" (+18 more) | property sets: Pset_Draughting
          6 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 160 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 160 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "6.12.2", "6.23.0", "6.22.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          8 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          15 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "8.19.1" | material: layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "8.19.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "6.2.16", "6.2.18" | property sets: Pset_Draughting
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "5.5.0", "5.21.0", "5.10.0" (+1 more) | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2012" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "5.70.6", "5.70.8", "6.27.10" (+2 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | property sets: Pset_Draughting
          31 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "8.18.0", "8.15.0", "8.14.0" (+14 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "8.7.4", "8.7.6" | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "8.7.33", "6.3.0", "6.4.0" (+1 more) | property sets: Pset_Draughting
          18 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "8.18.4", "8.15.4", "8.14.4" (+6 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "5.60.13" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "5.61.5", "6.2.20" | property sets: Pset_Draughting
          9 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "6.27.13", "6.5.8", "6.6.7" (+5 more) | property sets: Pset_Draughting
          3 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.2.2", "5.5.2" | material: layers "ML-1600x400-Insulation fire 30 mm-50" ("Layer-1600x400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | names: "5.2.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "5.3.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "5.4.0" | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "5.6.8", "5.36.8", "5.37.0" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "5.38.0", "5.39.0" | property sets: Pset_Draughting
          32 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.48.1", "5.48.3", "5.47.1" (+29 more) | material: layers "ML-Circular duct zinc plated 250 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 250 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          32 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.44.2", "5.44.5", "5.41.2" (+29 more) | material: layers "ML-Circular duct zinc plated 315 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 315 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          11 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "5.70.1", "5.70.4", "5.70.6" (+8 more) | material: layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          4 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "5.67.0", "6.9.4", "6.16.2" (+1 more) | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "5.56.0", "5.60.16", "5.64.4" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-3200x1200-Insulation fire 30 mm-50" ("Layer-3200x1200" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          5 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.2.1", "6.2.6", "6.2.7" (+2 more) | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "6.2.11" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2032" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2031" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "6.6.2", "6.25.0", "6.13.16" (+5 more) | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.25.2", "6.25.4" | material: layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "6.25.2" | property sets: Pset_Draughting
          15 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "6.25.6", "6.25.8", "6.26.1" (+12 more) | material: layers "ML-Circular duct zinc plated 100 mm" ("Layer-Circular duct zinc plated 100 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          9 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "6.25.7", "6.26.0", "6.24.10" (+6 more) | property sets: Pset_Draughting
          1 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "6.24.0" | property sets: Pset_Draughting
          7 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "6.24.2", "6.12.4", "6.9.6" (+4 more) | property sets: Pset_Draughting
          5 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "6.11.0", "6.10.0", "6.23.8" (+1 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "6.13.13" | property sets: Pset_Draughting
          4 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 630 mm" ("Layer-Circular duct zinc plated 630 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2801" | property sets: Pset_Draughting
          1 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom" | property sets: Pset_Draughting
      IFCBUILDINGSTOREY "Ventilation 2nd floor" | COMPLEX | elevation 5.5 | description "Ventilation 2nd floor"
        contains 4626 elements
          9 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "15.1.1", "15.1.4", "15.1.6" (+6 more) | material: layers "ML-400x300-Insulation fire 30 mm-50" ("Layer-400x300" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-400x300" ("Layer-400x300" 0.002) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          3080 x IFCDISTRIBUTIONPORT
          13 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "15.1.0", "15.2.0", "16.26.7" (+8 more) | property sets: Pset_Draughting
          13 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "15.1.2", "16.26.3", "16.35.4" (+10 more) | property sets: Pset_Draughting
          3 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "15.1.4", "16.25.2", "16.26.5" | property sets: Pset_Draughting
          20 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "IT2099" | names: "15.1.6", "17.1.0", "17.1.1" (+17 more) | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "15.1.7", "15.1.9", "16.25.4" (+6 more) | property sets: Pset_Draughting
          10 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "15.1.11", "16.35.16", "16.36.0" (+7 more) | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "15.2.2", "15.3.0", "14.3.24" (+1 more) | property sets: Pset_Draughting
          7 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "15.3.1", "13.10.1", "13.10.4" (+4 more) | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028); layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.1.2" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | names: "16.1.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "16.2.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.3.0" | property sets: Pset_Draughting
          13 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.25.2", "16.25.4", "16.25.5" (+10 more) | material: layers "ML-Rectangular duct zinc plated 500x400-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 500x400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          5 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "16.25.0", "16.4.0", "18.1.0" (+2 more) | property sets: Pset_Draughting
          5 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "16.25.8", "16.4.4", "16.5.0" (+2 more) | property sets: Pset_Draughting
          3 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "16.26.0", "16.35.11", "13.1.24" | property sets: Pset_Draughting
          45 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.26.5", "16.26.7", "16.26.8" (+42 more) | material: layers "ML-Rectangular duct zinc plated 400x300-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 400x300" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Rectangular duct zinc plated 400x300" ("Layer-Rectangular duct zinc plated 400x300" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "16.26.11" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | names: "16.27.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.28.0" | property sets: Pset_Draughting
          24 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.32.2", "16.32.5", "16.29.2" (+21 more) | material: layers "ML-Circular duct zinc plated 315 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 315 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          38 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "16.32.0", "16.32.2", "16.29.0" (+35 more) | property sets: Pset_Draughting
          25 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.32.3", "16.29.3", "16.38.3" (+22 more) | property sets: Pset_Draughting
          116 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.33.1", "16.30.1", "16.34.1" (+113 more) | material: layers "ML-Circular duct zinc plated 250 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 250 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          11 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "16.33.0", "16.30.0", "16.34.0" (+7 more) | property sets: Pset_Draughting
          6 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "16.35.6", "16.4.2", "16.16.4" (+3 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "16.35.8", "13.1.21" | property sets: Pset_Draughting
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "16.35.13", "13.1.26" | material: layers "ML-Rectangular duct zinc plated 600x200-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated 600x200" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.37.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.6.0" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | names: "16.17.0", "19.4.8" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.18.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "16.9.0" | property sets: Pset_Draughting
          22 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "16.23.0", "16.23.2", "16.24.0" (+19 more) | property sets: Pset_Draughting
          23 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "16.24.4", "16.21.0", "16.20.0" (+20 more) | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-1200 x 400-Insulation fire 30 mm-50" ("Layer-1200 x 400" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2002" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2003" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          11 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "17.1.1", "17.1.2", "17.1.4" (+8 more) | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028); layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          7 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "17.1.2", "17.1.4", "18.1.5" (+4 more) | property sets: Pset_Draughting
          61 x IFCFLOWTREATMENTDEVICE | type IFCDUCTSILENCERTYPE "SI2000" | names: "18.1.3", "11.10.10", "11.9.6" (+58 more) | property sets: Pset_Draughting
          20 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "17.3.3", "17.3.5", "17.3.7" (+17 more) | material: layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028); layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "17.3.2", "17.3.4", "17.2.0" (+5 more) | property sets: Pset_Draughting
          4 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "17.3.6", "17.2.16", "18.3.5" (+1 more) | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-500x600-Insulation fire 30 mm-50" ("Layer-500x600" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "19.3.0" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "19.13.0" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "19.5.0", "14.3.15" | property sets: Pset_Draughting
          58 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "19.5.4", "19.5.6", "19.5.9" (+55 more) | material: layers "ML-Circular duct zinc plated 400 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 400 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 400 mm" ("Layer-Circular duct zinc plated 400 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          73 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "19.5.3", "19.8.0", "19.6.0" (+70 more) | property sets: Pset_Draughting
          92 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "19.5.5", "19.14.0", "11.1.0" (+89 more) | property sets: Pset_Draughting
          25 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "19.8.1", "19.8.4", "19.8.7" (+22 more) | material: layers "ML-Circular duct zinc plated 315 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 315 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 315 mm" ("Layer-Circular duct zinc plated 315 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          37 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "19.9.1", "19.10.1", "19.6.1" (+34 more) | material: layers "ML-Circular duct zinc plated 250 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 250 mm" 0.002, "Layer-Insulation fire 30 mm" 0.05); layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "11.1.2", "12.1.6" | property sets: Pset_Draughting
          11 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "11.1.12", "12.1.10", "12.1.12" (+8 more) | property sets: Pset_Draughting
          9 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "11.1.14", "11.1.16", "11.1.18" (+6 more) | property sets: Pset_Draughting
          13 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "11.1.20", "11.1.22", "11.1.39" (+10 more) | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "11.1.28", "12.1.22" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "11.1.44" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          39 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "12.5.0", "12.5.2", "12.2.0" (+36 more) | property sets: Pset_Draughting
          171 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "12.7.1", "12.4.1", "12.3.1" (+168 more) | material: layers "ML-Circular duct zinc plated 200 mm" ("Layer-Circular duct zinc plated 200 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          21 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "12.7.0", "12.4.0", "12.3.0" (+18 more) | property sets: Pset_Draughting
          55 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "12.17.1", "12.17.3", "12.17.5" (+52 more) | material: layers "ML-Circular duct zinc plated 125 mm" ("Layer-Circular duct zinc plated 125 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          10 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "12.17.4", "12.16.12", "12.15.8" (+7 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "11.11.4" | property sets: Pset_Draughting
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "11.11.8" | property sets: Pset_Draughting
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "11.12.1" | material: layers "ML-Circular duct zinc plated 100 mm" ("Layer-Circular duct zinc plated 100 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "11.12.0" | property sets: Pset_Draughting
          59 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "11.10.1", "11.10.3", "11.10.5" (+56 more) | material: layers "ML-Circular duct zinc plated 160 mm" ("Layer-Circular duct zinc plated 160 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          11 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "11.10.8", "11.9.2", "11.8.2" (+8 more) | property sets: Pset_Draughting
          9 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2701" | names: "11.10.14", "11.9.10", "11.8.10" (+6 more) | property sets: Pset_Draughting
          9 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "12.16.8", "12.15.2", "12.14.2" (+6 more) | property sets: Pset_Draughting
          48 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "10.1.1", "10.1.3", "10.1.4" (+45 more) | material: layers "ML-Circular duct zinc plated 500 mm" ("Layer-Circular duct zinc plated 500 mm" 0.028); layers "ML-Circular duct zinc plated 500 mm-Insulation fire 30 mm-50" ("Layer-Circular duct zinc plated 500 mm" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "10.1.38", "8.1.38" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "10.1.55" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "10.1.57", "8.1.53" | property sets: Pset_Draughting
          2 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "8.19.12", "20.1.4" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "CH2000" | names: "10.20.4", "8.4.6" | property sets: Pset_Draughting
          34 x IFCFLOWCONTROLLER | type IFCDAMPERTYPE "DM2001" | names: "10.20.9", "10.21.0", "8.20.4" (+31 more) | property sets: Pset_Draughting
          2 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "10.20.15", "10.21.6" | property sets: Pset_Draughting
          18 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2201" | names: "8.20.11", "8.18.6", "8.17.6" (+15 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2601" | names: "10.4.11" | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TA2000" | names: "14.3.12", "13.1.8" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "LI2000" | names: "13.3.0" | property sets: Pset_Draughting
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "13.10.8", "13.10.10" | property sets: Pset_Draughting
          1 x IFCFLOWMOVINGDEVICE | type IFCFANTYPE "FA2000" | names: "20.1.0"
          1 x IFCENERGYCONVERSIONDEVICE | type IFCAIRTOAIRHEATRECOVERYTYPE "DH2001" | names: "20.1.2" | property sets: Pset_Draughting
          36 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | names: "20.1.12", "20.1.18", "20.1.22" (+33 more) | property sets: Pset_Draughting
          36 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2001" | names: "20.1.16", "20.1.20", "20.1.24" (+33 more) | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct" | names: "20.1.158" | property sets: Pset_Draughting
          36 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | names: "20.37.1", "20.36.1", "20.35.1" (+33 more) | material: layers "ML-Circular duct zinc plated 80 mm" ("Layer-Circular duct zinc plated 80 mm" 0.002) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          36 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GV2901" | names: "20.37.1", "20.36.0", "20.35.0" (+33 more) | property sets: Pset_Draughting, Pset_FlowTerminalAirTerminal
          3 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-4700x1300-Insulation fire 30 mm-50" ("Layer-4700x1300" 0.002, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "TP2004" | property sets: Pset_Draughting
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Circular duct zinc plated 250 mm" ("Layer-Circular duct zinc plated 250 mm" 0.028) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS0000" | material: layers "ML-Rectangular duct zinc plated free dim-Insulation fire 30 mm-50" ("Layer-Rectangular duct zinc plated free dim" 0.028, "Layer-Insulation fire 30 mm" 0.05) | property sets: Pset_Draughting, Pset_FlowSegmentDuctSegment
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "VenEndDuct"

Types
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_300_1100" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "TP2002" | element type "TP020101_002_Y713302_1095" | JUNCTION | 6 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP020101_003_Y713302_1107" | JUNCTION | 7 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI020101_000_Y718312_1081" | OBSTRUCTION | 24 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid rectangular zink plated"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_1100" | RIGIDSEGMENT | 19 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y722302_1010" | BEND | 147 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1300_500" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_500" | RIGIDSEGMENT | 15 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1217_500_400" | RIGIDSEGMENT | 60 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 500x400"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1067" | OBSTRUCTION | 8 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_400" | RIGIDSEGMENT | 92 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_Y714302_1007" | JUNCTION | 37 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 200x100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y722302_1029" | BEND | 45 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y722302_1118" | BEND | 15 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1224_630_400" | RIGIDSEGMENT | 20 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 630 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903155833_1003_400_300" | RIGIDSEGMENT | 23 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "400x300"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP020101_001_Y713302_1008" | JUNCTION | 5 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903160157_1004_300_1100" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "1200 x 400"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_400_1200" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903160347_1005_300_600" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "400x700"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903160627_1006_400_500" | RIGIDSEGMENT | 8 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "500x600"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225_400_500" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1014" | TRANSITION | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220" | RIGIDSEGMENT | 78 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y7223025_1010" | BEND | 184 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI010101_000_Y74000 5_1035" | ROUND | 111 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer circular type L= 1000mm"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1040" | BALANCINGDAMPER | 22 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1230_600_500" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 600x500"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1018" | TRANSITION | 5 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_500_500" | RIGIDSEGMENT | 12 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER020101_000_Y712300_1016" | BEND | 62 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rectangular zink plated bend 90°"
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI020101_000_Y74100 5_1037" | RECTANGULAR | 20 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer rectangular type L= 1000mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1231_160_500" | RIGIDSEGMENT | 25 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 160 mm"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1042" | BALANCINGDAMPER | 19 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1022" | JUNCTION | 36 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1025" | TRANSITION | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1232" | RIGIDSEGMENT | 179 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 125 mm"
  IFCAIRTERMINALTYPE "GV2701" | element type "GV510101_701_Y2613000012_1024" | GRILLE | 20 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB KGEB m.KGEZ-01 125 mm connection"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1231" | RIGIDSEGMENT | 117 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 160 mm"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1028" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y7223025_1029" | BEND | 109 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-270903162740_1031" | GRILLE | 24 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø125"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1032" | JUNCTION | 19 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1068" | OBSTRUCTION | 50 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225" | RIGIDSEGMENT | 112 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV530101_201_GV-270903194008_1123" | GRILLE | 13 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB evacuation valve rectangular w. rect. chamber 400 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903163809_1043_1300_400" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "1300x400"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARS010101_000_Y716312_1017" | TRANSITION | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition from rectangular to circular free dim"
  IFCDAMPERTYPE "DM2002" | element type "DM010101_002_Y2320311_1038" | BALANCINGDAMPER | 2 occurrences | description "Zink plated zonebox 500 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903164256_1047_1300_500" | RIGIDSEGMENT | 8 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "1300x500"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1111" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1233_1200_500" | RIGIDSEGMENT | 8 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 1200x500"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_Y714302_1055" | JUNCTION | 15 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 200x100"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1058" | JUNCTION | 26 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_400_500" | RIGIDSEGMENT | 4 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER020101_000_Y712300_1120" | BEND | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rectangular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1113" | TRANSITION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_500_400" | RIGIDSEGMENT | 5 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1053" | BALANCINGDAMPER | 30 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1234_400_300" | RIGIDSEGMENT | 104 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 400x300"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1235_315_300" | RIGIDSEGMENT | 72 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 315 mm"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1059" | JUNCTION | 116 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1218_250_300" | RIGIDSEGMENT | 171 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 250 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-270903165423_1061" | GRILLE | 103 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø250"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1062" | BALANCINGDAMPER | 9 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER020101_000_Y712300_1063" | BEND | 7 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rectangular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER020101_000_Y712300_1065" | BEND | 32 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rectangular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1064" | JUNCTION | 6 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-011003112611_1179_1600_1000" | RIGIDSEGMENT | 4 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "1600x1000"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1045" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1236_1200_400" | RIGIDSEGMENT | 14 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 1200x400"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP010101_003_Y723302_1183" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1072" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1021" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1235_315_400" | RIGIDSEGMENT | 36 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 315 mm"
  IFCAIRTERMINALTYPE "GV2701" | element type "GV510101_701_Y2613000020_1071" | GRILLE | 1 occurrence | property sets: Pset_AirTerminalTypeCommon | description "ABB KGEB m.KGEZ-01 200 mm connection"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1231_160_400" | RIGIDSEGMENT | 6 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 160 mm"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1077" | JUNCTION | 14 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1112" | TRANSITION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1237" | RIGIDSEGMENT | 27 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 100 mm"
  IFCAIRTERMINALTYPE "GV2701" | element type "GV510101_701_Y2613000010_1076" | GRILLE | 12 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB KGEB m.KGEZ-01 100 mm connection"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1078" | BALANCINGDAMPER | 28 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI010101_000_Y74000 3_1079" | ROUND | 8 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer circular type L= 600mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1235" | RIGIDSEGMENT | 60 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 315 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1226_1000_500" | RIGIDSEGMENT | 16 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 1000x500"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1066" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1084" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1082" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1218_250_500" | RIGIDSEGMENT | 12 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 250 mm"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1088" | BALANCINGDAMPER | 4 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1085" | JUNCTION | 64 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1238_200_500" | RIGIDSEGMENT | 9 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 200 mm"
  IFCAIRTERMINALTYPE "GV2301" | element type "GV010101_301_Y251327_1087" | GRILLE | 8 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Cylo 4-way 100mm"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1090" | OBSTRUCTION | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1235_315_500" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 315 mm"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1093" | BALANCINGDAMPER | 39 occurrences | description "Zink plated irisdamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1224" | RIGIDSEGMENT | 8 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 630 mm"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1097" | JUNCTION | 5 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCAIRTERMINALTYPE "GV2801" | element type "GV080101_801_GV-270903174820_1099" | GRILLE | 4 occurrences | property sets: Pset_AirTerminalTypeCommon | description "Grating for rectangular duct, zink plated"
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1218" | RIGIDSEGMENT | 84 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 250 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1238" | RIGIDSEGMENT | 219 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 200 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-270903180035_1100_1600_400" | RIGIDSEGMENT | 9 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "1600x400"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-270903180214_1102" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 1000x400"
  IFCAIRTOAIRHEATRECOVERYTYPE "DH2001" | element type "DH010101_001_Y51003_1108" | HEATPIPE | 2 occurrences | description "Zink plated enclosing"
  IFCDAMPERTYPE "DM2012" | element type "DM020101_012_Y2323311_1109" | BALANCINGDAMPER | 1 occurrence | description "Zink plated smokedamper 80 mm L=100"
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI020101_000_Y74100 4_1110" | RECTANGULAR | 2 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer rectangular type L= 900mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1000_400" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "TP2002" | element type "TP010101_002_Y723302_1106" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225_400_400" | RIGIDSEGMENT | 32 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCFANTYPE "GF2500" | element type "GF010101_500_ABB500_1168" | USERDEFINED | 1 occurrence | description "ABB Aggregate 500"
  IFCFANTYPE "GF2500" | element type "GF010101_500_ABB501_1169" | USERDEFINED | 1 occurrence | description "ABB Aggregate 501"
  IFCFANTYPE "GF2500" | element type "GF010101_500_ABB502_1170" | USERDEFINED | 1 occurrence | description "ABB Aggregate 502"
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI010101_000_Y74000 4_1171" | ROUND | 4 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer circular type L= 900mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1134" | OBSTRUCTION | 40 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-011003103525_1172_2600_1600" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "2600x1600"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1173" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1400_400" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-011003111201_1175_1700_600" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "1700x600"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP020101_003_Y713302_1129" | JUNCTION | 3 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP020101_003_Y713302_1223" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet negative free dim"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1600_400" | RIGIDSEGMENT | 5 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP020101_003_Y713302_1181" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1222_1000_600" | RIGIDSEGMENT | 8 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 1000x600"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_600" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225_400_600" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-011003115608_1186_2000_1500" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "2000x1500"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-011003120137_1187" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 1000x1000"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1000_1000" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_700_1000" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-011003123905_1189" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 3300x500"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_3300_800" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_3300_1300" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP010101_003_Y723302_1193" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1224_630_500" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 630 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-011003111303_1176" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 1600x400"
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | ENTRY | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-011003131012_1194" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 1600x600"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_3300_500" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1219_1600_600" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated free dim"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCPIPEFITTINGTYPE "IT2099" | element type "IT010101_099_S17140_1002" | BEND | 24 occurrences | description "Insulation fire 30 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV530101_201_GV-270903165027_1052" | GRILLE | 14 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB evacuation valve rectangular w. rect. chamber 250 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1239_600_300" | RIGIDSEGMENT | 4 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 600x300"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1115" | TRANSITION | 7 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1094" | JUNCTION | 29 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "LI2000" | element type "LI010101_000_Y728322_1116" | OBSTRUCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Lid circular zink plated 1250mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-270903183310_1117" | GRILLE | 13 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø160"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1012" | TRANSITION | 3 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1231_160_300" | RIGIDSEGMENT | 6 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 160 mm"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP010101_004_Y724302_1104" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular tee-part 63 mm"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225_400_300" | RIGIDSEGMENT | 15 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-270903163106_1033" | GRILLE | 6 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø400"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_300" | RIGIDSEGMENT | 15 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP020101_001_Y713302_1122" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TASR020101_000_Y716312_1121" | TRANSITION | 3 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDAMPERTYPE "DM2012" | element type "DM020101_012_Y2323311_1057" | BALANCINGDAMPER | 1 occurrence | description "Zink plated smokedamper 80 mm L=100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y7223025_1118" | BEND | 15 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1125" | TRANSITION | 4 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_Y255324_1126" | GRILLE | 5 occurrences | property sets: Pset_AirTerminalTypeCommon | description "Supply valve rectangular w. rect. chamber 125 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_Y255324_1127" | GRILLE | 2 occurrences | property sets: Pset_AirTerminalTypeCommon | description "Supply valve rectangular w. rect. chamber 125 mm"
  IFCDUCTFITTINGTYPE "TP2002" | element type "TP020101_002_Y713302_1130" | JUNCTION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_Y714302_1128" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 200x100"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP010101_003_Y723302_1132" | JUNCTION | 3 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1218_250_400" | RIGIDSEGMENT | 32 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 250 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-270903204726_1133" | GRILLE | 25 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø200"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-280903140003_1135_3200_1200" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "3200x1200"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1220_500_1200" | RIGIDSEGMENT | 5 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 500 mm"
  IFCDUCTFITTINGTYPE "TA2000" | element type "TASR020101_000_Y716312_1113" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCAIRTERMINALTYPE "GV2032" | element type "GV610101_032_GV-280903140837_1137" | GRILLE | 1 occurrence | property sets: Pset_AirTerminalTypeCommon | description "Evacuation chamber with grating right"
  IFCAIRTERMINALTYPE "GV2031" | element type "GV610101_031_GV-280903141312_1138" | GRILLE | 1 occurrence | property sets: Pset_AirTerminalTypeCommon | description "Evacuation chamber with grating right"
  IFCDAMPERTYPE "DM2001" | element type "DM010101_001_Y2323311_1139" | BALANCINGDAMPER | 1 occurrence | description "Zink plated irisdamper 80 mm L=100"
  IFCAIRTERMINALTYPE "GV2701" | element type "GV510101_701_Y2613000016_1020" | GRILLE | 14 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB KGEB m.KGEZ-01 160 mm connection"
  IFCDUCTFITTINGTYPE "CH2000" | element type "CHS010101_000_Y726302_1141" | TRANSITION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular transistion zink plated > 800"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP020101_001_Y713302_1163" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive 200x100"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSILENCERTYPE "SI2000" | element type "SI020101_000_Y74100 3_1142" | RECTANGULAR | 3 occurrences | property sets: Pset_DuctSilencerTypeCommon | description "Silencer rectangular type L= 600mm"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1121" | TRANSITION | 3 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTFITTINGTYPE "TP2003" | element type "TP010101_003_Y723302_1143" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TA2000" | element type "TARR020101_000_Y716312_1146" | TRANSITION | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Transition - recangular to rectangular 200x100"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_Y711312_1240_600_200" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Rectangular duct zinc plated 600x200"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "TP2002" | element type "TP020101_002_Y713302_1228" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular eccentric outlet positive free dim"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1225_400_1100" | RIGIDSEGMENT | 20 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 400 mm"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_Y714302_1229" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 500x400"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y7223025_1148" | BEND | 2 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV030101_201_GV-280903162327_1149" | GRILLE | 1 occurrence | property sets: Pset_AirTerminalTypeCommon | description "ABB Supply valve Ø315"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1152" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCAIRTERMINALTYPE "GV2201" | element type "GV530101_201_GV-280903170629_1151" | GRILLE | 18 occurrences | property sets: Pset_AirTerminalTypeCommon | description "ABB evacuation valve rectangular w. rect. chamber 200 mm"
  IFCAIRTERMINALTYPE "GV2601" | element type "GV060101_601_Y251334_1153" | GRILLE | 1 occurrence | property sets: Pset_AirTerminalTypeCommon | description "Chamber with diffuser 100 mm connection right"
  IFCDUCTFITTINGTYPE "LI2000" | OBSTRUCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCFANTYPE "FA2000" | element type "FA010101_000_Y610000_1157" | 1 occurrence | description "Radial fan zink plated"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010101_000_Y722302_1156" | BEND | 36 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular zink plated bend 90°"
  IFCDUCTFITTINGTYPE "TP2001" | element type "TP010101_001_Y723302_1158" | JUNCTION | 36 occurrences | property sets: Pset_DuctFittingTypeCommon | description "Circular outlet 63 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1241_80_300" | RIGIDSEGMENT | 36 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 80 mm"
  IFCAIRTERMINALTYPE "GV2901" | element type "GV070101_901_Y251300_1160" | GRILLE | 36 occurrences | property sets: Pset_AirTerminalTypeCommon | description "Control valve 100 mm connection"
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS020101_000_SS-280903180310_1161_4700_1300" | RIGIDSEGMENT | 3 occurrences | property sets: Pset_DuctSegmentTypeCommon | description "4700x1300"
  IFCDUCTFITTINGTYPE "TP2004" | element type "TP020101_004_TP-011003134931_1195" | JUNCTION | 1 occurrence | property sets: Pset_DuctFittingTypeCommon | description "Rektangular tee-part 3300x1300"
  IFCDUCTFITTINGTYPE "VenEndDuct" | EXIT | 1 occurrence | property sets: Pset_DuctFittingTypeCommon
  IFCDUCTSEGMENTTYPE "SS0000" | element type "SS010101_000_Y721322_1218_250_1300" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_DuctSegmentTypeCommon | description "Circular duct zinc plated 250 mm"
  IFCDUCTFITTINGTYPE "VenEndDuct" | CONNECTOR | 1 occurrence | property sets: Pset_DuctFittingTypeCommon

Property sets
  Storey quantities | quantities | on 6 objects (6 IFCBUILDINGSTOREY)
    TotalHeight = 2.75 [METRE]
  Storey quantities | quantities | on 2 objects (2 IFCBUILDINGSTOREY)
    TotalHeight = 0. [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 16 objects (16 IFCFLOWSEGMENT)
    Length = 0.1963584721088409 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 16 objects (16 IFCFLOWSEGMENT)
    Length = 0.5492211580276489 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Length = 0.09999847412109375 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 14 objects (14 IFCFLOWSEGMENT)
    Length = 3.5 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 14 objects (14 IFCFLOWSEGMENT)
    Length = 0.8558141589164734 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 14 objects (14 IFCFLOWSEGMENT)
    Length = 0.2839778065681458 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 14 objects (14 IFCFLOWSEGMENT)
    Length = 0.1097831726074219 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 13 objects (13 IFCFLOWSEGMENT)
    Length = 0.5 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment: 1369 more contents on 1753 objects not shown
  Pset_Draughting | properties | on 2098 objects (1181 IFCFLOWSEGMENT, 753 IFCFLOWFITTING, 84 IFCFLOWCONTROLLER, 80 IFCFLOWTREATMENTDEVICE)
    Colour: Red = 255 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0361 KANALNETT" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 1260 objects (686 IFCFLOWSEGMENT, 435 IFCFLOWFITTING, 71 IFCFLOWCONTROLLER, 68 IFCFLOWTREATMENTDEVICE)
    Colour: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 255 (IFCINTEGER)
    LayerName = "0361 KANALNETT" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 273 objects (273 IFCFLOWTERMINAL)
    Colour: Red = 255 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0100 STANDARD" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 222 objects (218 IFCFLOWFITTING, 4 IFCFLOWTERMINAL)
    Colour: Red = 0 (IFCINTEGER); Green = 240 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0100 STANDARD" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 45 objects (45 IFCFLOWTERMINAL)
    Colour: Red = 0 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 255 (IFCINTEGER)
    LayerName = "0100 STANDARD" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 3 objects (3 IFCFLOWMOVINGDEVICE)
    Colour: Red = 0 (IFCINTEGER); Green = 240 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "0360" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Colour: Red = 255 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "BATTERI" (IFCIDENTIFIER)
  Pset_Draughting | properties | on 2 objects (1 IFCFLOWCONTROLLER, 1 IFCFLOWSEGMENT)
    Colour: Red = 255 (IFCINTEGER); Green = 0 (IFCINTEGER); Blue = 0 (IFCINTEGER)
    LayerName = "KANALNETT" (IFCIDENTIFIER)
  Pset_Draughting: 2 more contents on 2 objects not shown
  Pset_FlowTerminalAirTerminal | properties | on 12 objects (12 IFCFLOWTERMINAL)
    AirflowType in {"RETURNAIR"} (IFCTEXT)
  Pset_FlowTerminalAirTerminal | properties | on 9 objects (9 IFCFLOWTERMINAL)
    AirflowType in {"SUPPLYAIR"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 7 type objects
    NominalDiameterOrWidth = [0.5] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 6 type objects
    NominalDiameterOrWidth = [0.4] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 5 type objects
    NominalDiameterOrWidth = [0.25] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 4 type objects
    NominalDiameterOrWidth = [0.16] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 4 type objects
    NominalDiameterOrWidth = [0.315] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 3 type objects
    NominalDiameterOrWidth = [0.63] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 2 type objects
    NominalDiameterOrWidth = [0.3] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [1.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 2 type objects
    NominalDiameterOrWidth = [1.3] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.5] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon: 33 more contents on 0 objects not shown
  Pset_DuctFittingTypeCommon | properties | on 37 type objects
    NominalDiameterOrWidth = [0.5] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 18 type objects
    NominalDiameterOrWidth = [0.4] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.3] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 12 type objects
    NominalDiameterOrWidth = [0.63] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 11 type objects
    NominalDiameterOrWidth = [0.4] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 7 type objects
    NominalDiameterOrWidth = [0.4] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.5] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 4 type objects
    NominalDiameterOrWidth = [0.3] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [1.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 4 type objects
    NominalDiameterOrWidth = [0.5] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.4] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 3 type objects
    NominalDiameterOrWidth = [0.3, 0.5, 0.3] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [1.1, 0.5, 1.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon: 69 more contents on 0 objects not shown
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = FALSE (IFCBOOLEAN)
    Length = 1. (IFCLENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = TRUE (IFCBOOLEAN)
    Length = 1. (IFCLENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = FALSE (IFCBOOLEAN)
    Length = 0.6 (IFCLENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = TRUE (IFCBOOLEAN)
    Length = 0.9 (IFCLENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = FALSE (IFCBOOLEAN)
    Length = 0.9 (IFCLENGTHMEASURE) [METRE]
    Shape in {"ROUND"} (IFCTEXT)
  Pset_DuctSilencerTypeCommon | properties | on 1 type object
    HasExteriorInsulation = TRUE (IFCBOOLEAN)
    Length = 0.6 (IFCLENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_AirTerminalTypeCommon | properties | on 2 type objects
    AirFlowrateRange = 0.12 .. 0.12 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.03141592815518379 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 2 type objects
    AirFlowrateRange = 0. .. 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.1256637126207352 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.0388 .. 0.0388 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.01227184664458036 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.0541 .. 0.0541 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.01227184664458036 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.5388 .. 0.5388 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.1256637126207352 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.15 .. 0.15 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.04908738657832146 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.0972 .. 0.0972 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.03141592815518379 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon | properties | on 1 type object
    AirFlowrateRange = 0.0277 .. 0.0277 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    NeckArea = 0.007853982038795948 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_AirTerminalTypeCommon: 11 more contents on 0 objects not shown